Version: V2.0 | Release Date: 2022-11-18

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Process Data Formatting]
[Menus]

R45C
Vendor ID | 451 (0x01c3) |
Vendor Name | Banner Engineering Corporation
Vendor Text | More Sensors. More Solutions.
Vendor URL | www.bannerengineering.com/io-link
Device ID | 659471 (0x0a100f)
DeviceFamily | R45C Series
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x0001 (Device Profile: Smart Sensor), 0x0011 (Device Profile: ?Unknown?), 0x4000 (Common Application Profile: ?Unknown?), 0x8000 (Function Class: Device Identification), 0x8003 (Function Class: Device Diagnosis), 0x800d (Function Class: ?Unknown?)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: yes
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 7.6 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_0 with 1 octet on-request data OPERATE = TYPE_2_V with 1 octet on-request data ISDU supported
Device Variant | R45C-KUU-UUQ
--- | ---
Description | Dual Analog to IO-Link converter - Voltage
Product ID | R45C-KUU-UUQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
Device Variant | R45C-KII-IIQ
Description | Dual Analog to IO-Link converter - Current
Product ID | R45C-KII-IIQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q

[Top]

## ProcessData id=PD_ProcessDataWithSignal (condition V_Vendor_Specific_Configuration.1 == 0)

## ProcessDataIn "Process Data Input" id=PD_ProcessDataIn

bit length: 64
data type: 64-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Measurement Value 1 | The measurement device value
5 | 0 | 32-bit Integer |  |  |  |  |  | Measurement Value 2 | The channel 2 measurement device value

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 5 | 5 | 5 | 5
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## ProcessDataOut "Process Data Output" id=PD_ProcessDataOut

bit length: 64
data type: 64-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Analog Output Value 1 | The value to output to the channel 1 analog output
2 | 0 | 32-bit Integer |  |  |  |  |  | Analog Output Value 2 | The value to output to the channel 2 analog output

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## ProcessData id=PD_ProcessDataWithDMS (condition V_Vendor_Specific_Configuration.1 == 1)

## ProcessDataIn "Process Data Input" id=PD_ProcessDataInDMS

bit length: 64
data type: 64-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 48 | 16-bit Integer |  |  |  |  |  | Measurement Value 1 | The measurement device value
2 | 40 | 8-bit Integer |  |  |  |  |  | Measurement Scale 1 | The channel 1 measurement device scale
4 | 32 | Boolean |  |  |  |  |  | SSC1.1 - Switching Signal | Indicates the detection status of an object or measurement value within a window.
5 | 16 | 16-bit Integer |  |  |  |  |  | Measurement Value 2 | The channel 2 measurement device value
6 | 8 | 8-bit Integer |  |  |  |  |  | Measurement Scale 2 | The channel 2 measurement device scale
8 | 0 | Boolean |  |  |  |  |  | SSC2.1 - Switching Signal | Indicates the detection status of an object or measurement value within a window.

Octet 0

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 1
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 1
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | 2
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 3

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4

Octet 4

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 5
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 5

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 5
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 6

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 6
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 7

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 8

## ProcessDataOut "Process Data Output" id=PD_ProcessDataOutDMS

bit length: 64
data type: 64-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Analog Output Value 1 | The value to output to the channel 1 analog output
2 | 0 | 32-bit Integer |  |  |  |  |  | Analog Output Value 2 | The value to output to the channel 2 analog output

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 65 = SP1 Single Value Teach, 67 = SP1 Two Value Teach TP1, 68 = SP1 Two Value Teach TP2, 71 = SP1 Dynamic Teach Start, 72 = SP1 Dynamic Teach Stop, 79 = SP1 Exit Teach, 130 = Restore Factory Settings, 162 = Discovery Start, 163 = Discovery Stop, 164 = Reset Output Event |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 65 = SP1 Single Value Teach, 67 = SP1 Two Value Teach TP1, 68 = SP1 Two Value Teach TP2, 71 = SP1 Dynamic Teach Start, 72 = SP1 Dynamic Teach Stop, 79 = SP1 Exit Teach, 130 = Restore Factory Settings, 162 = Discovery Start, 163 = Discovery Stop, 164 = Reset Output Event
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  |  |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure, 5..255 = Reserved
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

data type: Array[6] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 6 | 6 |

## Standard Variable "Process Data Input" index=40 id=V_ProcessDataInput

data type: see ProcessDataIn!
access rights: ro
dynamic

## Standard Variable "Process Data Output" index=41 id=V_ProcessDataOutput

data type: see ProcessDataOut!
access rights: ro
dynamic
[Top]

## Variable "SSC1.BDC1 Setpoints" index=60 id=V_BDC1_Setpoints

description: The reference value used for sensor switching (See IOL Smart Sensor Profile 9.2.5)
data type: 64-bit Record (subindex access not supported)
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Setpoint SP1 | SP1 switch point.
2 | 0 | 32-bit Integer |  |  |  |  |  | Setpoint SP2 | SP2 switch point.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "SSC1.BDC1 Configuration" index=61 id=V_BDC1_Configuration

description: Parameter coding of the Setpoint and Switchpoint parameter. (See IOL Smart Sensor Profile 9.2.6)
data type: 32-bit Record
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 8-bit UInteger | 0 = Light Operate (LO) - Discrete Output is On while target is detected | 0 |  |  |  | Switchpoint Logic | Set LO/DO selection
2 | 16 | 8-bit UInteger | 2 = Window Mode | 2 |  |  |  | BDC Mode | Defines how the binary switching information is created depending on Setpoint parameters (SP1, SP2) and the current measurement value
3 | 0 | 16-bit UInteger |  |  |  |  |  | Hysteresis | The hysteresis value for the switchpoint.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "Port 1 Mirroring Configuration" index=64 id=V_Port_Mirroring_Configuration_1

description: Port mirroring configuration options.
data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Output Enable | Enable mirroring over output analog channel.
2 | 8 | 8-bit UInteger | 0 = Analog In 1, 1 = Analog In 2 | 0 |  |  |  | Mirroring Input Port Selection | Input port to mirror over output analog channel.

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 2 | 1 |
element bit | 7 - 0 | 7 - 0 |

## Variable "Port 2 Mirroring Configuration" index=65 id=V_Port_Mirroring_Configuration_2

description: Port mirroring configuration options.
data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Output Enable | Enable mirroring over output analog channel.
2 | 8 | 8-bit UInteger | 0 = Analog In 1, 1 = Analog In 2 | 1 |  |  |  | Mirroring Input Port Selection | Input port to mirror over output analog channel.

octet | 0 | 1 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 2 | 1 |
element bit | 7 - 0 | 7 - 0 |

## Variable "All-time Run Time" index=69 id=V_AllTimeRunTime

description: A read only run time counter (in hours) that tracks the total time the sensor has been running since manufacture
data type: 32-bit Record (subindex access not supported)
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time" index=70 id=V_ResetableRunTime

description: A read / write run time counter (in hours) that can be monitored or set by the user
data type: 32-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Pulse Frequency Configuration" index=71 id=V_PulseFrequencyConfiguration

description: Configuration of pulse frequency ranges.
data type: 64-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 100..45000 | 100 |  |  |  | Near Frequency | The frequency corresponding to a target at the near limit of the sensing range.
2 | 32 | 32-bit Integer | 100..45000 | 600 |  |  |  | Far Frequency | The frequency corresponding to a target at the far limit of the sensing range.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 1
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Pulse Frequency LOS Frequency" index=72 id=V_PulseFrequencyLOSFrequency

description: Frequency used to indicate Loss-of-Signal
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 50..45000 | 50 |  |  |  | Pulse Frequency LOS Frequency | Frequency used to indicate Loss-of-Signal

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Vendor Specific Configuration" index=76 id=V_Vendor_Specific_Configuration

description: Vendor Specific Configuration
data type: 56-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Analog Value, 1 = Digital Measuring Sensor | 0 |  |  |  | Process Data Input Configuration | The available Process Data Input Data Map Selections
2 | 8 | 16-bit UInteger |  | 200 |  |  |  | IOL Filter Time | Time to average IOL process data measurement between updates.
3 | 24 | 8-bit UInteger | 0 = Hold, 1 = Low, 2 = High | 1 |  |  |  | SSC1.PDO Outside Valid Range (POVR) | Output value sensor will output when process data output value is not within the allowable range.
4 | 32 | 8-bit UInteger | 0 = Hold, 1 = Low, 2 = High | 1 |  |  |  | SSC2.PDO Outside Valid Range (POVR) | Output value sensor will output when process data output value is not within the allowable range.
5 | 40 | 8-bit UInteger | 0 = Disabled, 1 = Pulse Frequency Modulation | 0 |  |  |  | Secondary Output Function | The function of the secondary output channel
6 | 48 | 8-bit UInteger | 0 = Analog In 1, 1 = Analog In 2 | 0 |  |  |  | PFM Input Port Selection | Analog input channel to use to determine PFM output frequency.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 |
bit offset | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 6 | 5 | 4 | 3 | 2 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "All-time Run Time Event Time" index=78 id=V_AllTimeRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Event indicating the corresponding configured running time has elapsed.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time Event Time" index=79 id=V_ResetableRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Model Type" index=86 id=V_ModelType

description: Track whether current or voltage model is connected
data type: 8-bit UInteger
allowed values: 0 = Voltage, 1 = Current
default value: 0
access rights: ro

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Variable "SSC2.BDC1 Setpoints" index=16396 id=V_SSC2_BDC1_Setpoints

description: The reference value used for sensor switching (See IOL Smart Sensor Profile 9.2.5)
data type: 64-bit Record (subindex access not supported)
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Setpoint SP1 | SP1 switch point.
2 | 0 | 32-bit Integer |  |  |  |  |  | Setpoint SP2 | SP2 switch point.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "SSC2.BDC1 Configuration" index=16397 id=V_SSC2_BDC1_Configuration

description: Parameter coding of the Setpoint and Switchpoint parameter. (See IOL Smart Sensor Profile 9.2.6)
data type: 32-bit Record
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 8-bit UInteger | 0 = Light Operate (LO) - Discrete Output is On while target is detected | 0 |  |  |  | Switchpoint Logic | Set LO/DO selection
2 | 16 | 8-bit UInteger | 2 = Window Mode | 2 |  |  |  | BDC Mode | Defines how the binary switching information is created depending on Setpoint parameters (SP1, SP2) and the current measurement value
3 | 0 | 16-bit UInteger |  |  |  |  |  | Hysteresis | The hysteresis value for the switchpoint.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "MDC Descriptor 1" index=16512 id=V_MDCDescriptor

description: Measuring Data Channel Descriptor - refer to Smart Sensor Profile 2nd Ed.
data type: 88-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 56 | 32-bit Integer |  |  |  |  |  | MDC Descr - Lower Limit |
2 | 24 | 32-bit Integer |  |  |  |  |  | MDC Descr - Upper Limit |
3 | 8 | 16-bit UInteger | 1209 = A, 1240 = V |  |  |  |  | MDC Descr - Unit |
4 | 0 | 8-bit Integer |  |  |  |  |  | MDC Descr - Scale |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 4 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "MDC Descriptor 2" index=16513 id=V_MDCDescriptor_2

description: Measuring Data Channel Descriptor - refer to Smart Sensor Profile 2nd Ed.
data type: 88-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 56 | 32-bit Integer |  |  |  |  |  | MDC Descr - Lower Limit |
2 | 24 | 32-bit Integer |  |  |  |  |  | MDC Descr - Upper Limit |
3 | 8 | 16-bit UInteger | 1209 = A, 1240 = V |  |  |  |  | MDC Descr - Unit |
4 | 0 | 8-bit Integer |  |  |  |  |  | MDC Descr - Scale |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 4 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
25376 (0x6320) | Error | Parameter error | Check data sheet and values
36000 (0x8ca0) | Warning | All-time Run Time Event | Event indicating the corresponding configured running time has elapsed.
36001 (0x8ca1) | Warning | Resetable Run Time Event | Event indicating the corresponding configured running time has elapsed.

[Top]

## Process Data Formatting

Formatting for Process Data id=PD_ProcessDataIn
Subindex 1:

Formatting for Process Data id=PD_ProcessDataInDMS
Subindex 1:

Formatting for Process Data id=PD_ProcessDataOut
Subindex 1:

Formatting for Process Data id=PD_ProcessDataOutDMS
Subindex 1:

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_ApplicationSpecificTag

Parameter Menu
V_Vendor_Specific_Configuration.Process Data Input Configuration, ro

Observation Menu
Model Type
V_ModelType
If V_ModelType = 0:
Process Data Input
V_ProcessDataInput.1 * 0.001 V
V_ProcessDataInput.5 * 0.001 V
If V_ModelType = 0:
Process Data Output
V_ProcessDataOutput.1 * 0.001 V
V_ProcessDataOutput.2 * 0.001 V
If V_ModelType = 1:
Process Data Input
V_ProcessDataInput.1 * 1E-06 A
V_ProcessDataInput.5 * 1E-06 A
If V_ModelType = 1:
Process Data Output
V_ProcessDataOutput.1 * 1E-06 A
V_ProcessDataOutput.2 * 1E-06 A

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameter Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
Access Locks
V_DeviceAccessLocks.Local Parameterization Lock
V_DeviceAccessLocks.Local User Interface Lock
If V_ModelType = 0:
SSC1.BDC1 Setpoints
V_BDC1_Setpoints.Setpoint SP1 * 0.001 V
V_BDC1_Setpoints.Setpoint SP2 * 0.001 V
If V_ModelType = 1:
SSC1.BDC1 Setpoints
V_BDC1_Setpoints.Setpoint SP1 * 1E-06 A
V_BDC1_Setpoints.Setpoint SP2 * 1E-06 A
If V_ModelType = 0:
SSC1.BDC1 Configuration
V_BDC1_Configuration.Hysteresis * 0.001 V
If V_ModelType = 1:
SSC1.BDC1 Configuration
V_BDC1_Configuration.Hysteresis * 1E-06 A
If V_ModelType = 0:
SSC2.BDC1 Setpoints
V_SSC2_BDC1_Setpoints.Setpoint SP1 * 0.001 V
V_SSC2_BDC1_Setpoints.Setpoint SP2 * 0.001 V
If V_ModelType = 1:
SSC2.BDC1 Setpoints
V_SSC2_BDC1_Setpoints.Setpoint SP1 * 1E-06 A
V_SSC2_BDC1_Setpoints.Setpoint SP2 * 1E-06 A
If V_ModelType = 0:
SSC2.BDC1 Configuration
V_SSC2_BDC1_Configuration.Hysteresis * 0.001 V
If V_ModelType = 1:
SSC2.BDC1 Configuration
V_SSC2_BDC1_Configuration.Hysteresis * 1E-06 A
Vendor Specific Configuration
V_Vendor_Specific_Configuration.Process Data Input Configuration
V_Vendor_Specific_Configuration.IOL Filter Time ms
V_Vendor_Specific_Configuration.SSC1.PDO Outside Valid Range (POVR)
V_Vendor_Specific_Configuration.SSC2.PDO Outside Valid Range (POVR)
V_Vendor_Specific_Configuration.Secondary Output Function
V_Vendor_Specific_Configuration.PFM Input Port Selection
Port 1 Mirroring Configuration
V_Port_Mirroring_Configuration_1
Port 2 Mirroring Configuration
V_Port_Mirroring_Configuration_2
Pulse Frequency Configuration
V_PulseFrequencyConfiguration.Near Frequency Hz
V_PulseFrequencyConfiguration.Far Frequency Hz
V_PulseFrequencyLOSFrequency.Pulse Frequency LOS Frequency Hz

Observation Menu
Model Type
V_ModelType
If V_ModelType = 0:
Process Data Input
V_ProcessDataInput.1 * 0.001 V
V_ProcessDataInput.5 * 0.001 V
If V_ModelType = 0:
Process Data Output
V_ProcessDataOutput.1 * 0.001 V
V_ProcessDataOutput.2 * 0.001 V
If V_ModelType = 1:
Process Data Input
V_ProcessDataInput.1 * 1E-06 A
V_ProcessDataInput.5 * 1E-06 A
If V_ModelType = 1:
Process Data Output
V_ProcessDataOutput.1 * 1E-06 A
V_ProcessDataOutput.2 * 1E-06 A

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
If V_ModelType = 0:
Measuring Data Channel 1
V_MDCDescriptor.MDC Descr - Lower Limit * 0.001 V
V_MDCDescriptor.MDC Descr - Upper Limit * 0.001 V
V_MDCDescriptor.MDC Descr - Scale
V_MDCDescriptor.MDC Descr - Unit
If V_ModelType = 0:
Measuring Data Channel 2
V_MDCDescriptor_2.MDC Descr - Lower Limit * 0.001 V
V_MDCDescriptor_2.MDC Descr - Upper Limit * 0.001 V
V_MDCDescriptor_2.MDC Descr - Scale
V_MDCDescriptor_2.MDC Descr - Unit
If V_ModelType = 1:
Measuring Data Channel 1
V_MDCDescriptor.MDC Descr - Lower Limit * 1E-06 A
V_MDCDescriptor.MDC Descr - Upper Limit * 1E-06 A
V_MDCDescriptor.MDC Descr - Scale
V_MDCDescriptor.MDC Descr - Unit
If V_ModelType = 1:
Measuring Data Channel 2
V_MDCDescriptor_2.MDC Descr - Lower Limit * 1E-06 A
V_MDCDescriptor_2.MDC Descr - Upper Limit * 1E-06 A
V_MDCDescriptor_2.MDC Descr - Scale
V_MDCDescriptor_2.MDC Descr - Unit
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameter Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
Access Locks
V_DeviceAccessLocks.Local Parameterization Lock
V_DeviceAccessLocks.Local User Interface Lock
If V_ModelType = 0:
SSC1.BDC1 Setpoints
V_BDC1_Setpoints.Setpoint SP1 * 0.001 V
V_BDC1_Setpoints.Setpoint SP2 * 0.001 V
If V_ModelType = 1:
SSC1.BDC1 Setpoints
V_BDC1_Setpoints.Setpoint SP1 * 1E-06 A
V_BDC1_Setpoints.Setpoint SP2 * 1E-06 A
If V_ModelType = 0:
SSC1.BDC1 Configuration
V_BDC1_Configuration.Hysteresis * 0.001 V
If V_ModelType = 1:
SSC1.BDC1 Configuration
V_BDC1_Configuration.Hysteresis * 1E-06 A
If V_ModelType = 0:
SSC2.BDC1 Setpoints
V_SSC2_BDC1_Setpoints.Setpoint SP1 * 0.001 V
V_SSC2_BDC1_Setpoints.Setpoint SP2 * 0.001 V
If V_ModelType = 1:
SSC2.BDC1 Setpoints
V_SSC2_BDC1_Setpoints.Setpoint SP1 * 1E-06 A
V_SSC2_BDC1_Setpoints.Setpoint SP2 * 1E-06 A
If V_ModelType = 0:
SSC2.BDC1 Configuration
V_SSC2_BDC1_Configuration.Hysteresis * 0.001 V
If V_ModelType = 1:
SSC2.BDC1 Configuration
V_SSC2_BDC1_Configuration.Hysteresis * 1E-06 A
Vendor Specific Configuration
V_Vendor_Specific_Configuration.Process Data Input Configuration
V_Vendor_Specific_Configuration.IOL Filter Time ms
V_Vendor_Specific_Configuration.SSC1.PDO Outside Valid Range (POVR)
V_Vendor_Specific_Configuration.SSC2.PDO Outside Valid Range (POVR)
V_Vendor_Specific_Configuration.Secondary Output Function
V_Vendor_Specific_Configuration.PFM Input Port Selection
Port 1 Mirroring Configuration
V_Port_Mirroring_Configuration_1
Port 2 Mirroring Configuration
V_Port_Mirroring_Configuration_2
Pulse Frequency Configuration
V_PulseFrequencyConfiguration.Near Frequency Hz
V_PulseFrequencyConfiguration.Far Frequency Hz
V_PulseFrequencyLOSFrequency.Pulse Frequency LOS Frequency Hz

Observation Menu
Model Type
V_ModelType
If V_ModelType = 0:
Process Data Input
V_ProcessDataInput.1 * 0.001 V
V_ProcessDataInput.5 * 0.001 V
If V_ModelType = 0:
Process Data Output
V_ProcessDataOutput.1 * 0.001 V
V_ProcessDataOutput.2 * 0.001 V
If V_ModelType = 1:
Process Data Input
V_ProcessDataInput.1 * 1E-06 A
V_ProcessDataInput.5 * 1E-06 A
If V_ModelType = 1:
Process Data Output
V_ProcessDataOutput.1 * 1E-06 A
V_ProcessDataOutput.2 * 1E-06 A

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
If V_ModelType = 0:
Measuring Data Channel 1
V_MDCDescriptor.MDC Descr - Lower Limit * 0.001 V
V_MDCDescriptor.MDC Descr - Upper Limit * 0.001 V
V_MDCDescriptor.MDC Descr - Scale
V_MDCDescriptor.MDC Descr - Unit
If V_ModelType = 0:
Measuring Data Channel 2
V_MDCDescriptor_2.MDC Descr - Lower Limit * 0.001 V
V_MDCDescriptor_2.MDC Descr - Upper Limit * 0.001 V
V_MDCDescriptor_2.MDC Descr - Scale
V_MDCDescriptor_2.MDC Descr - Unit
If V_ModelType = 1:
Measuring Data Channel 1
V_MDCDescriptor.MDC Descr - Lower Limit * 1E-06 A
V_MDCDescriptor.MDC Descr - Upper Limit * 1E-06 A
V_MDCDescriptor.MDC Descr - Scale
V_MDCDescriptor.MDC Descr - Unit
If V_ModelType = 1:
Measuring Data Channel 2
V_MDCDescriptor_2.MDC Descr - Lower Limit * 1E-06 A
V_MDCDescriptor_2.MDC Descr - Upper Limit * 1E-06 A
V_MDCDescriptor_2.MDC Descr - Scale
V_MDCDescriptor_2.MDC Descr - Unit
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.