Version: V1.0 | Release Date: 2023-11-01

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Menus]

R130C
Vendor ID | 451 (0x01c3) |
Vendor Name | Banner Engineering Corporation
Vendor Text | More Sensors. More Solutions.
Vendor URL | www.bannerengineering.com/io-link
Device ID | 659475 (0x0a1013)
DeviceFamily | R130C Series
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x4000 (Common Application Profile: Identification and Diagnosis)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: yes
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 3.3 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_0 with 1 octet on-request data OPERATE = TYPE_2_6 with 1 octet on-request data ISDU supported
Device Variant | R130C-8P22-KQ
--- | ---
Description | PNP to IO-Link converter
Product ID | R130C-8P22-KQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q

[Top]

## ProcessData id=PD_ProcessData (condition V_Vendor_Specific_Configuration.Process Data Grouping = 0)

## ProcessDataIn "Process Data Input" id=PD_ProcessDataIn

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | Boolean | false = Inactive, true = Active |  |  |  |  | Port1 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
2 | 9 | Boolean | false = Inactive, true = Active |  |  |  |  | Port1 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
3 | 10 | Boolean | false = Inactive, true = Active |  |  |  |  | Port2 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
4 | 11 | Boolean | false = Inactive, true = Active |  |  |  |  | Port2 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
5 | 12 | Boolean | false = Inactive, true = Active |  |  |  |  | Port3 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
6 | 13 | Boolean | false = Inactive, true = Active |  |  |  |  | Port3 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
7 | 14 | Boolean | false = Inactive, true = Active |  |  |  |  | Port4 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
8 | 15 | Boolean | false = Inactive, true = Active |  |  |  |  | Port4 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
9 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Port5 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
10 | 1 | Boolean | false = Inactive, true = Active |  |  |  |  | Port5 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
11 | 2 | Boolean | false = Inactive, true = Active |  |  |  |  | Port6 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
12 | 3 | Boolean | false = Inactive, true = Active |  |  |  |  | Port6 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
13 | 4 | Boolean | false = Inactive, true = Active |  |  |  |  | Port7 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
14 | 5 | Boolean | false = Inactive, true = Active |  |  |  |  | Port7 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
15 | 6 | Boolean | false = Inactive, true = Active |  |  |  |  | Port8 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
16 | 7 | Boolean | false = Inactive, true = Active |  |  |  |  | Port8 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

## ProcessDataOut "Process Data Output" id=PD_ProcessDataOut

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | Boolean | false = Off, true = On |  |  |  |  | Port1 Discrete1 Output State | true (1) = Discrete1 Output Active
2 | 9 | Boolean | false = Off, true = On |  |  |  |  | Port1 Discrete2 Output State | true (1) = Discrete2 Output Active
3 | 10 | Boolean | false = Off, true = On |  |  |  |  | Port2 Discrete1 Output State | true (1) = Discrete1 Output Active
4 | 11 | Boolean | false = Off, true = On |  |  |  |  | Port2 Discrete2 Output State | true (1) = Discrete2 Output Active
5 | 12 | Boolean | false = Off, true = On |  |  |  |  | Port3 Discrete1 Output State | true (1) = Discrete1 Output Active
6 | 13 | Boolean | false = Off, true = On |  |  |  |  | Port3 Discrete2 Output State | true (1) = Discrete2 Output Active
7 | 14 | Boolean | false = Off, true = On |  |  |  |  | Port4 Discrete1 Output State | true (1) = Discrete1 Output Active
8 | 15 | Boolean | false = Off, true = On |  |  |  |  | Port4 Discrete2 Output State | true (1) = Discrete2 Output Active
9 | 0 | Boolean | false = Off, true = On |  |  |  |  | Port5 Discrete1 Output State | true (1) = Discrete1 Output Active
10 | 1 | Boolean | false = Off, true = On |  |  |  |  | Port5 Discrete2 Output State | true (1) = Discrete2 Output Active
11 | 2 | Boolean | false = Off, true = On |  |  |  |  | Port6 Discrete1 Output State | true (1) = Discrete1 Output Active
12 | 3 | Boolean | false = Off, true = On |  |  |  |  | Port6 Discrete2 Output State | true (1) = Discrete2 Output Active
13 | 4 | Boolean | false = Off, true = On |  |  |  |  | Port7 Discrete1 Output State | true (1) = Discrete1 Output Active
14 | 5 | Boolean | false = Off, true = On |  |  |  |  | Port7 Discrete2 Output State | true (1) = Discrete2 Output Active
15 | 6 | Boolean | false = Off, true = On |  |  |  |  | Port8 Discrete1 Output State | true (1) = Discrete1 Output Active
16 | 7 | Boolean | false = Off, true = On |  |  |  |  | Port8 Discrete2 Output State | true (1) = Discrete2 Output Active

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

## ProcessData id=PD_ProcessDataByChannel (condition V_Vendor_Specific_Configuration.Process Data Grouping = 1)

## ProcessDataIn "Process Data Input" id=PD_ProcessDataInByChannel

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | Boolean | false = Inactive, true = Active |  |  |  |  | Port1 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
2 | 9 | Boolean | false = Inactive, true = Active |  |  |  |  | Port2 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
3 | 10 | Boolean | false = Inactive, true = Active |  |  |  |  | Port3 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
4 | 11 | Boolean | false = Inactive, true = Active |  |  |  |  | Port4 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
5 | 12 | Boolean | false = Inactive, true = Active |  |  |  |  | Port5 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
6 | 13 | Boolean | false = Inactive, true = Active |  |  |  |  | Port6 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
7 | 14 | Boolean | false = Inactive, true = Active |  |  |  |  | Port7 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
8 | 15 | Boolean | false = Inactive, true = Active |  |  |  |  | Port8 Discrete1 Input State | true (1) = Discrete1 Input Active. Note - even if Discrete1 is configured as an output, the active state will be reflected at the input
9 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Port1 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
10 | 1 | Boolean | false = Inactive, true = Active |  |  |  |  | Port2 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
11 | 2 | Boolean | false = Inactive, true = Active |  |  |  |  | Port3 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
12 | 3 | Boolean | false = Inactive, true = Active |  |  |  |  | Port4 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
13 | 4 | Boolean | false = Inactive, true = Active |  |  |  |  | Port5 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
14 | 5 | Boolean | false = Inactive, true = Active |  |  |  |  | Port6 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
15 | 6 | Boolean | false = Inactive, true = Active |  |  |  |  | Port7 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
16 | 7 | Boolean | false = Inactive, true = Active |  |  |  |  | Port8 Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

## ProcessDataOut "Process Data Output" id=PD_ProcessDataOutByChannel

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | Boolean | false = Off, true = On |  |  |  |  | Port1 Discrete1 Output State | true (1) = Discrete1 Output Active
2 | 9 | Boolean | false = Off, true = On |  |  |  |  | Port2 Discrete1 Output State | true (1) = Discrete1 Output Active
3 | 10 | Boolean | false = Off, true = On |  |  |  |  | Port3 Discrete1 Output State | true (1) = Discrete1 Output Active
4 | 11 | Boolean | false = Off, true = On |  |  |  |  | Port4 Discrete1 Output State | true (1) = Discrete1 Output Active
5 | 12 | Boolean | false = Off, true = On |  |  |  |  | Port5 Discrete1 Output State | true (1) = Discrete1 Output Active
6 | 13 | Boolean | false = Off, true = On |  |  |  |  | Port6 Discrete1 Output State | true (1) = Discrete1 Output Active
7 | 14 | Boolean | false = Off, true = On |  |  |  |  | Port7 Discrete1 Output State | true (1) = Discrete1 Output Active
8 | 15 | Boolean | false = Off, true = On |  |  |  |  | Port8 Discrete1 Output State | true (1) = Discrete2 Output Active
9 | 0 | Boolean | false = Off, true = On |  |  |  |  | Port1 Discrete2 Output State | true (1) = Discrete2 Output Active
10 | 1 | Boolean | false = Off, true = On |  |  |  |  | Port2 Discrete2 Output State | true (1) = Discrete2 Output Active
11 | 2 | Boolean | false = Off, true = On |  |  |  |  | Port3 Discrete2 Output State | true (1) = Discrete1 Output Active
12 | 3 | Boolean | false = Off, true = On |  |  |  |  | Port4 Discrete2 Output State | true (1) = Discrete2 Output Active
13 | 4 | Boolean | false = Off, true = On |  |  |  |  | Port5 Discrete2 Output State | true (1) = Discrete2 Output Active
14 | 5 | Boolean | false = Off, true = On |  |  |  |  | Port6 Discrete2 Output State | true (1) = Discrete2 Output Active
15 | 6 | Boolean | false = Off, true = On |  |  |  |  | Port7 Discrete2 Output State | true (1) = Discrete2 Output Active
16 | 7 | Boolean | false = Off, true = On |  |  |  |  | Port8 Discrete2 Output State | true (1) = Discrete2 Output Active

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

[Top]

## Standard Variable "Direct Parameters - Page 1" index=0 id=V_DirectParameters_1

description: Comprises the required parameters defining the communication characteristics and identifiers for device validation.
data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time | Communication: Current communication cycle duration used by the master. This value defines the process data cycle.
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time | Communication: Minimum communication cycle duration supported by the device. This value defines the lowest possible process data cycle.
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability | Communication: Information on the structure and the supported features of the communication messages.
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Revision ID | Communication: Identifier for the currently used communication protocol revision.
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length | Communication: Information on width and features of the process input data (Process Data from Device to Master).
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length | Communication: Information on width of the process output data (Process Data from Master to Device).
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 | Identification: Highest octet of the Vendor ID. Combined with the parameter Vendor ID 2, this parameter defines the 16-bit value of the unique Vendor ID as assigned by the IO-Link Community.
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 | Identification: Lowest octet of the Vendor ID. Combined with the parameter Vendor ID 1, this parameter defines the 16-bit value of the unique Vendor ID as assigned by the IO-Link Community.
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 | Identification: Highest octet of the Device ID. Combined with the parameters Device ID 2 and 3, this parameter defines the 24-bit value of the vendor-specific Device ID.
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 | Identification: Middle octet of the Device ID. Combined with the parameters Device ID 1 and 3, this parameter defines the 24-bit value of the vendor-specific Device ID.
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 | Identification: Lowest octet of the Device ID. Combined with the parameters Device ID 1 and 2, this parameter defines the 24-bit value of the vendor-specific Device ID.
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger |  |  | wo | X |  | System Command | Application: Command interface for devices without ISDU support. Validity and execution of commands are not confirmed.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters - Page 2" index=1 id=V_DirectParameters_2

description: A set of parameters for devices without ISDU support.
data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "System Command" index=2 id=V_SystemCommand

description: Command interface for applications. A positive acknowledge indicates the complete and correct finalization of the requested function.
data type: 8-bit UInteger
allowed values: 130 = Restore Factory Settings, 162 = Discovery Start, 163 = Discovery Stop, 164 = Reset All Metrics
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

description: The access to the device parameters can be restricted by setting appropriate flags within this parameter.
data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Parameter Write Access | This lock prevents the write access to all read/write parameters of the device except for the parameter 'Device Access Locks'.
2 | 1 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Data Storage | This lock prevents the write access to the device parameters via the data storage mechanism.
3 | 2 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Local Parameterization | This lock prevents the device settings from being changed via local operating elements on the device.
4 | 3 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Local User Interface | This lock prevents the access to the device settings and display via a local user interface. The user interface is disabled.

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

description: The vendor name that is assigned to a Vendor ID.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

description: Additional information about the vendor.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

description: Complete product name.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

description: Vendor-specific product or type identification (e.g., item number or model number).
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

description: Additional product information for the device.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

description: Unique, vendor-specific identifier of the individual device.
data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Revision" index=23 id=V_FirmwareRevision

description: Unique, vendor-specific identifier of the firmware revision of the individual device.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application-specific Tag" index=24 id=V_ApplicationSpecificTag

description: Possibility to mark a device with user- or application-specific information.
data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

description: Indicator for the current device condition and diagnosis state.
data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

description: List of all currently pending events in the device.
data type: Array[6] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 6 | 6 |

## Standard Variable "PD Input" index=40 id=V_ProcessDataInput

description: Last valid process input data of the device.
data type: see ProcessDataIn!
access rights: ro
dynamic

## Standard Variable "PD Output" index=41 id=V_ProcessDataOutput

description: Last valid process output data written to the device.
data type: see ProcessDataOut!
access rights: ro
dynamic
[Top]

## Variable "All-time Run Time" index=69 id=V_AllTimeRunTime

description: A read only run time counter (in hours) that tracks the total time the sensor has been running since manufacture
data type: 32-bit Record (subindex access not supported)
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time" index=70 id=V_ResetableRunTime

description: A read / write run time counter (in hours) that can be monitored or set by the user
data type: 32-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Vendor Specific Configuration" index=76 id=V_Vendor_Specific_Configuration

description: Vendor Specific Configuration
data type: 8-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Group by Port, 1 = Group by Channel | 0 |  |  |  | Process Data Grouping | Configure grouping of process data.

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "All-time Run Time Event Time" index=78 id=V_AllTimeRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Event indicating the corresponding configured running time has elapsed.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time Event Time" index=79 id=V_ResetableRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "IO Metrics Ports 1 to 4" index=80 id=V_IO_Metrics_Ports_1_to_4

description: IO Metrics Ports 1 to 4
data type: 1024-bit Record
access rights: ro
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer |  |  |  |  |  | Port1 Discrete1 Count |
2 | 32 | 32-bit Integer |  |  |  |  |  | Port1 Discrete1 Duration |
3 | 64 | 32-bit Integer |  |  |  |  |  | Port1 Discrete1 Events Per Minute |
4 | 96 | 32-bit Integer |  |  |  |  |  | Port1 Discrete1 Totalizer Counter |
5 | 128 | 32-bit Integer |  |  |  |  |  | Port1 Discrete2 Count |
6 | 160 | 32-bit Integer |  |  |  |  |  | Port1 Discrete2 Duration |
7 | 192 | 32-bit Integer |  |  |  |  |  | Port1 Discrete2 Events Per Minute |
8 | 224 | 32-bit Integer |  |  |  |  |  | Port1 Discrete2 Totalizer Counter |
9 | 256 | 32-bit Integer |  |  |  |  |  | Port2 Discrete1 Count |
10 | 288 | 32-bit Integer |  |  |  |  |  | Port2 Discrete1 Duration |
11 | 320 | 32-bit Integer |  |  |  |  |  | Port2 Discrete1 Events Per Minute |
12 | 352 | 32-bit Integer |  |  |  |  |  | Port2 Discrete1 Totalizer Counter |
13 | 384 | 32-bit Integer |  |  |  |  |  | Port2 Discrete2 Count |
14 | 416 | 32-bit Integer |  |  |  |  |  | Port2 Discrete2 Duration |
15 | 448 | 32-bit Integer |  |  |  |  |  | Port2 Discrete2 Events Per Minute |
16 | 480 | 32-bit Integer |  |  |  |  |  | Port2 Discrete2 Totalizer Counter |
17 | 512 | 32-bit Integer |  |  |  |  |  | Port3 Discrete1 Count |
18 | 544 | 32-bit Integer |  |  |  |  |  | Port3 Discrete1 Duration |
19 | 576 | 32-bit Integer |  |  |  |  |  | Port3 Discrete1 Events Per Minute |
20 | 608 | 32-bit Integer |  |  |  |  |  | Port3 Discrete1 Totalizer Counter |
21 | 640 | 32-bit Integer |  |  |  |  |  | Port3 Discrete2 Count |
22 | 672 | 32-bit Integer |  |  |  |  |  | Port3 Discrete2 Duration |
23 | 704 | 32-bit Integer |  |  |  |  |  | Port3 Discrete2 Events Per Minute |
24 | 736 | 32-bit Integer |  |  |  |  |  | Port3 Discrete2 Totalizer Counter |
25 | 768 | 32-bit Integer |  |  |  |  |  | Port4 Discrete1 Count |
26 | 800 | 32-bit Integer |  |  |  |  |  | Port4 Discrete1 Duration |
27 | 832 | 32-bit Integer |  |  |  |  |  | Port4 Discrete1 Events Per Minute |
28 | 864 | 32-bit Integer |  |  |  |  |  | Port4 Discrete1 Totalizer Counter |
29 | 896 | 32-bit Integer |  |  |  |  |  | Port4 Discrete2 Count |
30 | 928 | 32-bit Integer |  |  |  |  |  | Port4 Discrete2 Duration |
31 | 960 | 32-bit Integer |  |  |  |  |  | Port4 Discrete2 Events Per Minute |
32 | 992 | 32-bit Integer |  |  |  |  |  | Port4 Discrete2 Totalizer Counter |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 1023 - 1016 | 1015 - 1008 | 1007 - 1000 | 999 - 992 | 991 - 984 | 983 - 976 | 975 - 968 | 967 - 960
subindex | 32 | 32 | 32 | 32 | 31 | 31 | 31 | 31
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 959 - 952 | 951 - 944 | 943 - 936 | 935 - 928 | 927 - 920 | 919 - 912 | 911 - 904 | 903 - 896
subindex | 30 | 30 | 30 | 30 | 29 | 29 | 29 | 29
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 895 - 888 | 887 - 880 | 879 - 872 | 871 - 864 | 863 - 856 | 855 - 848 | 847 - 840 | 839 - 832
subindex | 28 | 28 | 28 | 28 | 27 | 27 | 27 | 27
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 831 - 824 | 823 - 816 | 815 - 808 | 807 - 800 | 799 - 792 | 791 - 784 | 783 - 776 | 775 - 768
subindex | 26 | 26 | 26 | 26 | 25 | 25 | 25 | 25
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 767 - 760 | 759 - 752 | 751 - 744 | 743 - 736 | 735 - 728 | 727 - 720 | 719 - 712 | 711 - 704
subindex | 24 | 24 | 24 | 24 | 23 | 23 | 23 | 23
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 703 - 696 | 695 - 688 | 687 - 680 | 679 - 672 | 671 - 664 | 663 - 656 | 655 - 648 | 647 - 640
subindex | 22 | 22 | 22 | 22 | 21 | 21 | 21 | 21
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 639 - 632 | 631 - 624 | 623 - 616 | 615 - 608 | 607 - 600 | 599 - 592 | 591 - 584 | 583 - 576
subindex | 20 | 20 | 20 | 20 | 19 | 19 | 19 | 19
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 575 - 568 | 567 - 560 | 559 - 552 | 551 - 544 | 543 - 536 | 535 - 528 | 527 - 520 | 519 - 512
subindex | 18 | 18 | 18 | 18 | 17 | 17 | 17 | 17
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 64 | 65 | 66 | 67 | 68 | 69 | 70 | 71
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448
subindex | 16 | 16 | 16 | 16 | 15 | 15 | 15 | 15
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 72 | 73 | 74 | 75 | 76 | 77 | 78 | 79
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384
subindex | 14 | 14 | 14 | 14 | 13 | 13 | 13 | 13
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 80 | 81 | 82 | 83 | 84 | 85 | 86 | 87
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320
subindex | 12 | 12 | 12 | 12 | 11 | 11 | 11 | 11
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 88 | 89 | 90 | 91 | 92 | 93 | 94 | 95
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256
subindex | 10 | 10 | 10 | 10 | 9 | 9 | 9 | 9
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 96 | 97 | 98 | 99 | 100 | 101 | 102 | 103
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192
subindex | 8 | 8 | 8 | 8 | 7 | 7 | 7 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 104 | 105 | 106 | 107 | 108 | 109 | 110 | 111
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128
subindex | 6 | 6 | 6 | 6 | 5 | 5 | 5 | 5
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 112 | 113 | 114 | 115 | 116 | 117 | 118 | 119
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 4 | 4 | 4 | 4 | 3 | 3 | 3 | 3
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 120 | 121 | 122 | 123 | 124 | 125 | 126 | 127
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 1
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "IO Metrics Ports 5 to 8" index=81 id=V_IO_Metrics_Ports_5_to_8

description: IO Metrics Ports 5 to 8 Values
data type: 1024-bit Record
access rights: ro
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer |  |  |  |  |  | Port5 Discrete1 Count |
2 | 32 | 32-bit Integer |  |  |  |  |  | Port5 Discrete1 Duration |
3 | 64 | 32-bit Integer |  |  |  |  |  | Port5 Discrete1 Events Per Minute |
4 | 96 | 32-bit Integer |  |  |  |  |  | Port5 Discrete1 Totalizer Counter |
5 | 128 | 32-bit Integer |  |  |  |  |  | Port5 Discrete2 Count |
6 | 160 | 32-bit Integer |  |  |  |  |  | Port5 Discrete2 Duration |
7 | 192 | 32-bit Integer |  |  |  |  |  | Port5 Discrete2 Events Per Minute |
8 | 224 | 32-bit Integer |  |  |  |  |  | Port5 Discrete2 Totalizer Counter |
9 | 256 | 32-bit Integer |  |  |  |  |  | Port6 Discrete1 Count |
10 | 288 | 32-bit Integer |  |  |  |  |  | Port6 Discrete1 Duration |
11 | 320 | 32-bit Integer |  |  |  |  |  | Port6 Discrete1 Events Per Minute |
12 | 352 | 32-bit Integer |  |  |  |  |  | Port6 Discrete1 Totalizer Counter |
13 | 384 | 32-bit Integer |  |  |  |  |  | Port6 Discrete2 Count |
14 | 416 | 32-bit Integer |  |  |  |  |  | Port6 Discrete2 Duration |
15 | 448 | 32-bit Integer |  |  |  |  |  | Port6 Discrete2 Events Per Minute |
16 | 480 | 32-bit Integer |  |  |  |  |  | Port6 Discrete2 Totalizer Counter |
17 | 512 | 32-bit Integer |  |  |  |  |  | Port7 Discrete1 Count |
18 | 544 | 32-bit Integer |  |  |  |  |  | Port7 Discrete1 Duration |
19 | 576 | 32-bit Integer |  |  |  |  |  | Port7 Discrete1 Events Per Minute |
20 | 608 | 32-bit Integer |  |  |  |  |  | Port7 Discrete1 Totalizer Counter |
21 | 640 | 32-bit Integer |  |  |  |  |  | Port7 Discrete2 Count |
22 | 672 | 32-bit Integer |  |  |  |  |  | Port7 Discrete2 Duration |
23 | 704 | 32-bit Integer |  |  |  |  |  | Port7 Discrete2 Events Per Minute |
24 | 736 | 32-bit Integer |  |  |  |  |  | Port7 Discrete2 Totalizer Counter |
25 | 768 | 32-bit Integer |  |  |  |  |  | Port8 Discrete1 Count |
26 | 800 | 32-bit Integer |  |  |  |  |  | Port8 Discrete1 Duration |
27 | 832 | 32-bit Integer |  |  |  |  |  | Port8 Discrete1 Events Per Minute |
28 | 864 | 32-bit Integer |  |  |  |  |  | Port8 Discrete1 Totalizer Counter |
29 | 896 | 32-bit Integer |  |  |  |  |  | Port8 Discrete2 Count |
30 | 928 | 32-bit Integer |  |  |  |  |  | Port8 Discrete2 Duration |
31 | 960 | 32-bit Integer |  |  |  |  |  | Port8 Discrete2 Events Per Minute |
32 | 992 | 32-bit Integer |  |  |  |  |  | Port8 Discrete2 Totalizer Counter |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 1023 - 1016 | 1015 - 1008 | 1007 - 1000 | 999 - 992 | 991 - 984 | 983 - 976 | 975 - 968 | 967 - 960
subindex | 32 | 32 | 32 | 32 | 31 | 31 | 31 | 31
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 959 - 952 | 951 - 944 | 943 - 936 | 935 - 928 | 927 - 920 | 919 - 912 | 911 - 904 | 903 - 896
subindex | 30 | 30 | 30 | 30 | 29 | 29 | 29 | 29
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 895 - 888 | 887 - 880 | 879 - 872 | 871 - 864 | 863 - 856 | 855 - 848 | 847 - 840 | 839 - 832
subindex | 28 | 28 | 28 | 28 | 27 | 27 | 27 | 27
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 831 - 824 | 823 - 816 | 815 - 808 | 807 - 800 | 799 - 792 | 791 - 784 | 783 - 776 | 775 - 768
subindex | 26 | 26 | 26 | 26 | 25 | 25 | 25 | 25
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 767 - 760 | 759 - 752 | 751 - 744 | 743 - 736 | 735 - 728 | 727 - 720 | 719 - 712 | 711 - 704
subindex | 24 | 24 | 24 | 24 | 23 | 23 | 23 | 23
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 703 - 696 | 695 - 688 | 687 - 680 | 679 - 672 | 671 - 664 | 663 - 656 | 655 - 648 | 647 - 640
subindex | 22 | 22 | 22 | 22 | 21 | 21 | 21 | 21
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 639 - 632 | 631 - 624 | 623 - 616 | 615 - 608 | 607 - 600 | 599 - 592 | 591 - 584 | 583 - 576
subindex | 20 | 20 | 20 | 20 | 19 | 19 | 19 | 19
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 575 - 568 | 567 - 560 | 559 - 552 | 551 - 544 | 543 - 536 | 535 - 528 | 527 - 520 | 519 - 512
subindex | 18 | 18 | 18 | 18 | 17 | 17 | 17 | 17
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 64 | 65 | 66 | 67 | 68 | 69 | 70 | 71
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448
subindex | 16 | 16 | 16 | 16 | 15 | 15 | 15 | 15
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 72 | 73 | 74 | 75 | 76 | 77 | 78 | 79
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384
subindex | 14 | 14 | 14 | 14 | 13 | 13 | 13 | 13
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 80 | 81 | 82 | 83 | 84 | 85 | 86 | 87
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320
subindex | 12 | 12 | 12 | 12 | 11 | 11 | 11 | 11
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 88 | 89 | 90 | 91 | 92 | 93 | 94 | 95
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256
subindex | 10 | 10 | 10 | 10 | 9 | 9 | 9 | 9
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 96 | 97 | 98 | 99 | 100 | 101 | 102 | 103
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192
subindex | 8 | 8 | 8 | 8 | 7 | 7 | 7 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 104 | 105 | 106 | 107 | 108 | 109 | 110 | 111
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128
subindex | 6 | 6 | 6 | 6 | 5 | 5 | 5 | 5
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 112 | 113 | 114 | 115 | 116 | 117 | 118 | 119
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 4 | 4 | 4 | 4 | 3 | 3 | 3 | 3
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 120 | 121 | 122 | 123 | 124 | 125 | 126 | 127
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 1
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Selectable Metric Reset" index=82 id=V_Selectable_Metric_Reset

description: User can select which channel / Channels to reset
data type: 528-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port1 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
2 | 1 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port1 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
3 | 2 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port2 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
4 | 3 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port2 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
5 | 4 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port3 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
6 | 5 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port3 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
7 | 6 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port4 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
8 | 7 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port4 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
9 | 8 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port5 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
10 | 9 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port5 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
11 | 10 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port6 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
12 | 11 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port6 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
13 | 12 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port7 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
14 | 13 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port7 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
15 | 14 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port8 Discrete1 | If set to [Reset], Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete1 Reset Count]
16 | 15 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port8 Discrete2 | If set to [Reset], Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port# Discrete2 Reset Count]
17 | 16 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port1 Discrete1 Reset Count |
18 | 48 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port1 Discrete2 Reset Count |
19 | 80 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port2 Discrete1 Reset Count |
20 | 112 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port2 Discrete2 Reset Count |
21 | 144 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port3 Discrete1 Reset Count |
22 | 176 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port3 Discrete2 Reset Count |
23 | 208 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port4 Discrete1 Reset Count |
24 | 240 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port4 Discrete2 Reset Count |
25 | 272 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port5 Discrete1 Reset Count |
26 | 304 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port5 Discrete2 Reset Count |
27 | 336 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port6 Discrete1 Reset Count |
28 | 368 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port6 Discrete2 Reset Count |
29 | 400 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port7 Discrete1 Reset Count |
30 | 432 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port7 Discrete2 Reset Count |
31 | 464 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port8 Discrete1 Reset Count |
32 | 496 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port8 Discrete2 Reset Count |

Octet 0

bit offset | 527 | 526 | 525 | 524 | 523 | 522 | 521 | 520
subindex | 32
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 1

bit offset | 519 | 518 | 517 | 516 | 515 | 514 | 513 | 512
subindex | 32
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 2

bit offset | 511 | 510 | 509 | 508 | 507 | 506 | 505 | 504
subindex | 32
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 3

bit offset | 503 | 502 | 501 | 500 | 499 | 498 | 497 | 496
subindex | 32
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 495 | 494 | 493 | 492 | 491 | 490 | 489 | 488
subindex | 31
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 5

bit offset | 487 | 486 | 485 | 484 | 483 | 482 | 481 | 480
subindex | 31
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 6

bit offset | 479 | 478 | 477 | 476 | 475 | 474 | 473 | 472
subindex | 31
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 7

bit offset | 471 | 470 | 469 | 468 | 467 | 466 | 465 | 464
subindex | 31
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 8

bit offset | 463 | 462 | 461 | 460 | 459 | 458 | 457 | 456
subindex | 30
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 9

bit offset | 455 | 454 | 453 | 452 | 451 | 450 | 449 | 448
subindex | 30
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 10

bit offset | 447 | 446 | 445 | 444 | 443 | 442 | 441 | 440
subindex | 30
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 11

bit offset | 439 | 438 | 437 | 436 | 435 | 434 | 433 | 432
subindex | 30
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 12

bit offset | 431 | 430 | 429 | 428 | 427 | 426 | 425 | 424
subindex | 29
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 13

bit offset | 423 | 422 | 421 | 420 | 419 | 418 | 417 | 416
subindex | 29
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 14

bit offset | 415 | 414 | 413 | 412 | 411 | 410 | 409 | 408
subindex | 29
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 15

bit offset | 407 | 406 | 405 | 404 | 403 | 402 | 401 | 400
subindex | 29
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 16

bit offset | 399 | 398 | 397 | 396 | 395 | 394 | 393 | 392
subindex | 28
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 17

bit offset | 391 | 390 | 389 | 388 | 387 | 386 | 385 | 384
subindex | 28
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 18

bit offset | 383 | 382 | 381 | 380 | 379 | 378 | 377 | 376
subindex | 28
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 19

bit offset | 375 | 374 | 373 | 372 | 371 | 370 | 369 | 368
subindex | 28
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 20

bit offset | 367 | 366 | 365 | 364 | 363 | 362 | 361 | 360
subindex | 27
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 21

bit offset | 359 | 358 | 357 | 356 | 355 | 354 | 353 | 352
subindex | 27
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 22

bit offset | 351 | 350 | 349 | 348 | 347 | 346 | 345 | 344
subindex | 27
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 23

bit offset | 343 | 342 | 341 | 340 | 339 | 338 | 337 | 336
subindex | 27
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 24

bit offset | 335 | 334 | 333 | 332 | 331 | 330 | 329 | 328
subindex | 26
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 25

bit offset | 327 | 326 | 325 | 324 | 323 | 322 | 321 | 320
subindex | 26
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 26

bit offset | 319 | 318 | 317 | 316 | 315 | 314 | 313 | 312
subindex | 26
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 27

bit offset | 311 | 310 | 309 | 308 | 307 | 306 | 305 | 304
subindex | 26
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 28

bit offset | 303 | 302 | 301 | 300 | 299 | 298 | 297 | 296
subindex | 25
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 29

bit offset | 295 | 294 | 293 | 292 | 291 | 290 | 289 | 288
subindex | 25
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 30

bit offset | 287 | 286 | 285 | 284 | 283 | 282 | 281 | 280
subindex | 25
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 31

bit offset | 279 | 278 | 277 | 276 | 275 | 274 | 273 | 272
subindex | 25
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 32

bit offset | 271 | 270 | 269 | 268 | 267 | 266 | 265 | 264
subindex | 24
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 33

bit offset | 263 | 262 | 261 | 260 | 259 | 258 | 257 | 256
subindex | 24
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 34

bit offset | 255 | 254 | 253 | 252 | 251 | 250 | 249 | 248
subindex | 24
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 35

bit offset | 247 | 246 | 245 | 244 | 243 | 242 | 241 | 240
subindex | 24
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 36

bit offset | 239 | 238 | 237 | 236 | 235 | 234 | 233 | 232
subindex | 23
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 37

bit offset | 231 | 230 | 229 | 228 | 227 | 226 | 225 | 224
subindex | 23
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 38

bit offset | 223 | 222 | 221 | 220 | 219 | 218 | 217 | 216
subindex | 23
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 39

bit offset | 215 | 214 | 213 | 212 | 211 | 210 | 209 | 208
subindex | 23
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 40

bit offset | 207 | 206 | 205 | 204 | 203 | 202 | 201 | 200
subindex | 22
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 41

bit offset | 199 | 198 | 197 | 196 | 195 | 194 | 193 | 192
subindex | 22
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 42

bit offset | 191 | 190 | 189 | 188 | 187 | 186 | 185 | 184
subindex | 22
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 43

bit offset | 183 | 182 | 181 | 180 | 179 | 178 | 177 | 176
subindex | 22
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 44

bit offset | 175 | 174 | 173 | 172 | 171 | 170 | 169 | 168
subindex | 21
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 45

bit offset | 167 | 166 | 165 | 164 | 163 | 162 | 161 | 160
subindex | 21
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 46

bit offset | 159 | 158 | 157 | 156 | 155 | 154 | 153 | 152
subindex | 21
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 47

bit offset | 151 | 150 | 149 | 148 | 147 | 146 | 145 | 144
subindex | 21
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 48

bit offset | 143 | 142 | 141 | 140 | 139 | 138 | 137 | 136
subindex | 20
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 49

bit offset | 135 | 134 | 133 | 132 | 131 | 130 | 129 | 128
subindex | 20
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 50

bit offset | 127 | 126 | 125 | 124 | 123 | 122 | 121 | 120
subindex | 20
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 51

bit offset | 119 | 118 | 117 | 116 | 115 | 114 | 113 | 112
subindex | 20
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 52

bit offset | 111 | 110 | 109 | 108 | 107 | 106 | 105 | 104
subindex | 19
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 53

bit offset | 103 | 102 | 101 | 100 | 99 | 98 | 97 | 96
subindex | 19
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 54

bit offset | 95 | 94 | 93 | 92 | 91 | 90 | 89 | 88
subindex | 19
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 55

bit offset | 87 | 86 | 85 | 84 | 83 | 82 | 81 | 80
subindex | 19
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 56

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | 18
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 57

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | 18
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 58

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 18
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 59

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 18
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 60

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | 17
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 61

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 17
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 62

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 17
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 63

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 17
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 64

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

Octet 65

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

## Variable "Port1 Configuration" index=87 id=V_Port1_Configuration

description: Port1 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Port2 Configuration" index=88 id=V_Port2_Configuration

description: Port2 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Port3 Configuration" index=89 id=V_Port3_Configuration

description: Port3 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Port4 Configuration" index=90 id=V_Port4_Configuration

description: Port4 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Port5 Configuration" index=91 id=V_Port5_Configuration

description: Port5 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Port6 Configuration" index=92 id=V_Port6_Configuration

description: Port6 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Port7 Configuration" index=93 id=V_Port7_Configuration

description: Port7 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Port8 Configuration" index=94 id=V_Port8_Configuration

description: Port8 Configuration
data type: 224-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete1 Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete1 Mirroring Port Selection |
7 | 96 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete1 Mirroring Channel Selection |
8 | 104 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete1 Mirroring Inversion |
9 | 112 | 8-bit UInteger | 1 = PNP Input, 3 = PNP Output with Pull Down | 3 |  |  |  | Discrete2 IO Selection |
10 | 120 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
11 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
12 | 160 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
13 | 192 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Discrete2 Mirroring Enable |
14 | 200 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Discrete2 Mirroring Port Selection |
15 | 208 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Discrete2 Mirroring Channel Selection |
16 | 216 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Discrete2 Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160
subindex | 16 | 15 | 14 | 13 | 12 | 12 | 12 | 12
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96
subindex | 11 | 11 | 11 | 11 | 10 | 9 | 8 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 6 | 5 | 4 | 4 | 4 | 4 | 3 | 3
element bit | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16

octet | 24 | 25 | 26 | 27 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 2 | 1 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Discrete Host Out Mirroring Configuration" index=95 id=V_Discrete_Host_Out_Mirroring_Configuration

description: Configuration parameters for mirroring Discrete1 or Discrete2 to White Host Out
data type: 48-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
2 | 8 | 8-bit UInteger | 0 = Port1, 1 = Port2, 2 = Port3, 3 = Port4, 4 = Port5, 5 = Port6, 6 = Port7, 7 = Port8 | 0 |  |  |  | Mirroring Port Selection |
3 | 16 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Mirroring Channel Selection |
4 | 24 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |
5 | 32 | 8-bit UInteger | 0 = NPN Output, 1 = PNP Output | 1 |  |  |  | Mirroring Polarity |
6 | 40 | 8-bit UInteger | 0 = Output Open Collector, 1 = Output Push Pull | 0 |  |  |  | Mirroring Output Type |

octet | 0 | 1 | 2 | 3 | 4 | 5 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 6 | 5 | 4 | 3 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
25376 (0x6320) | Error | Parameter error | Check datasheet and values
36000 (0x8ca0) | Warning | All-time Run Time Event | Event indicating the corresponding configured running time has elapsed.
36001 (0x8ca1) | Warning | Resetable Run Time Event | Event indicating the corresponding configured running time has elapsed.

[Top]

## Operator Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_ApplicationSpecificTag

Parameters Menu
V_Vendor_Specific_Configuration.Process Data Grouping, ro

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
IO Metrics Ports 1 to 4
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Totalizer Counter
IO Metrics Ports 5 to 8
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Totalizer Counter

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameters Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
Selectable Metric Reset
V_Selectable_Metric_Reset.Port1 Discrete1
V_Selectable_Metric_Reset.Port1 Discrete2
V_Selectable_Metric_Reset.Port2 Discrete1
V_Selectable_Metric_Reset.Port2 Discrete2
V_Selectable_Metric_Reset.Port3 Discrete1
V_Selectable_Metric_Reset.Port3 Discrete2
V_Selectable_Metric_Reset.Port4 Discrete1
V_Selectable_Metric_Reset.Port4 Discrete2
V_Selectable_Metric_Reset.Port5 Discrete1
V_Selectable_Metric_Reset.Port5 Discrete2
V_Selectable_Metric_Reset.Port6 Discrete1
V_Selectable_Metric_Reset.Port6 Discrete2
V_Selectable_Metric_Reset.Port7 Discrete1
V_Selectable_Metric_Reset.Port7 Discrete2
V_Selectable_Metric_Reset.Port8 Discrete1
V_Selectable_Metric_Reset.Port8 Discrete2
V_Selectable_Metric_Reset.Port1 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port1 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port2 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port2 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port3 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port3 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port4 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port4 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port5 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port5 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port6 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port6 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port7 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port7 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port8 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port8 Discrete2 Reset Count
Access Locks
V_DeviceAccessLocks.Local Parameterization
V_DeviceAccessLocks.Local User Interface
Vendor Specific Configuration
Port1 Configuration
V_Port1_Configuration.Discrete1 IO Selection
V_Port1_Configuration.Discrete1 Delay Mode
V_Port1_Configuration.Discrete1 Delay Timer 1 ms
V_Port1_Configuration.Discrete1 Delay Timer 2 ms
V_Port1_Configuration.Discrete1 Mirroring Enable
V_Port1_Configuration.Discrete1 Mirroring Port Selection
V_Port1_Configuration.Discrete1 Mirroring Channel Selection
V_Port1_Configuration.Discrete1 Mirroring Inversion
V_Port1_Configuration.Discrete2 IO Selection
V_Port1_Configuration.Discrete2 Delay Mode
V_Port1_Configuration.Discrete2 Delay Timer 1 ms
V_Port1_Configuration.Discrete2 Delay Timer 2 ms
V_Port1_Configuration.Discrete2 Mirroring Enable
V_Port1_Configuration.Discrete2 Mirroring Port Selection
V_Port1_Configuration.Discrete2 Mirroring Channel Selection
V_Port1_Configuration.Discrete2 Mirroring Inversion
Port2 Configuration
V_Port2_Configuration.Discrete1 IO Selection
V_Port2_Configuration.Discrete1 Delay Mode
V_Port2_Configuration.Discrete1 Delay Timer 1 ms
V_Port2_Configuration.Discrete1 Delay Timer 2 ms
V_Port2_Configuration.Discrete1 Mirroring Enable
V_Port2_Configuration.Discrete1 Mirroring Port Selection
V_Port2_Configuration.Discrete1 Mirroring Channel Selection
V_Port2_Configuration.Discrete1 Mirroring Inversion
V_Port2_Configuration.Discrete2 IO Selection
V_Port2_Configuration.Discrete2 Delay Mode
V_Port2_Configuration.Discrete2 Delay Timer 1 ms
V_Port2_Configuration.Discrete2 Delay Timer 2 ms
V_Port2_Configuration.Discrete2 Mirroring Enable
V_Port2_Configuration.Discrete2 Mirroring Port Selection
V_Port2_Configuration.Discrete2 Mirroring Channel Selection
V_Port2_Configuration.Discrete2 Mirroring Inversion
Port3 Configuration
V_Port3_Configuration.Discrete1 IO Selection
V_Port3_Configuration.Discrete1 Delay Mode
V_Port3_Configuration.Discrete1 Delay Timer 1 ms
V_Port3_Configuration.Discrete1 Delay Timer 2 ms
V_Port3_Configuration.Discrete1 Mirroring Enable
V_Port3_Configuration.Discrete1 Mirroring Port Selection
V_Port3_Configuration.Discrete1 Mirroring Channel Selection
V_Port3_Configuration.Discrete1 Mirroring Inversion
V_Port3_Configuration.Discrete2 IO Selection
V_Port3_Configuration.Discrete2 Delay Mode
V_Port3_Configuration.Discrete2 Delay Timer 1 ms
V_Port3_Configuration.Discrete2 Delay Timer 2 ms
V_Port3_Configuration.Discrete2 Mirroring Enable
V_Port3_Configuration.Discrete2 Mirroring Port Selection
V_Port3_Configuration.Discrete2 Mirroring Channel Selection
V_Port3_Configuration.Discrete2 Mirroring Inversion
Port4 Configuration
V_Port4_Configuration.Discrete1 IO Selection
V_Port4_Configuration.Discrete1 Delay Mode
V_Port4_Configuration.Discrete1 Delay Timer 1 ms
V_Port4_Configuration.Discrete1 Delay Timer 2 ms
V_Port4_Configuration.Discrete1 Mirroring Enable
V_Port4_Configuration.Discrete1 Mirroring Port Selection
V_Port4_Configuration.Discrete1 Mirroring Channel Selection
V_Port4_Configuration.Discrete1 Mirroring Inversion
V_Port4_Configuration.Discrete2 IO Selection
V_Port4_Configuration.Discrete2 Delay Mode
V_Port4_Configuration.Discrete2 Delay Timer 1 ms
V_Port4_Configuration.Discrete2 Delay Timer 2 ms
V_Port4_Configuration.Discrete2 Mirroring Enable
V_Port4_Configuration.Discrete2 Mirroring Port Selection
V_Port4_Configuration.Discrete2 Mirroring Channel Selection
V_Port4_Configuration.Discrete2 Mirroring Inversion
Port5 Configuration
V_Port5_Configuration.Discrete1 IO Selection
V_Port5_Configuration.Discrete1 Delay Mode
V_Port5_Configuration.Discrete1 Delay Timer 1 ms
V_Port5_Configuration.Discrete1 Delay Timer 2 ms
V_Port5_Configuration.Discrete1 Mirroring Enable
V_Port5_Configuration.Discrete1 Mirroring Port Selection
V_Port5_Configuration.Discrete1 Mirroring Channel Selection
V_Port5_Configuration.Discrete1 Mirroring Inversion
V_Port5_Configuration.Discrete2 IO Selection
V_Port5_Configuration.Discrete2 Delay Mode
V_Port5_Configuration.Discrete2 Delay Timer 1 ms
V_Port5_Configuration.Discrete2 Delay Timer 2 ms
V_Port5_Configuration.Discrete2 Mirroring Enable
V_Port5_Configuration.Discrete2 Mirroring Port Selection
V_Port5_Configuration.Discrete2 Mirroring Channel Selection
V_Port5_Configuration.Discrete2 Mirroring Inversion
Port6 Configuration
V_Port6_Configuration.Discrete1 IO Selection
V_Port6_Configuration.Discrete1 Delay Mode
V_Port6_Configuration.Discrete1 Delay Timer 1 ms
V_Port6_Configuration.Discrete1 Delay Timer 2 ms
V_Port6_Configuration.Discrete1 Mirroring Enable
V_Port6_Configuration.Discrete1 Mirroring Port Selection
V_Port6_Configuration.Discrete1 Mirroring Channel Selection
V_Port6_Configuration.Discrete1 Mirroring Inversion
V_Port6_Configuration.Discrete2 IO Selection
V_Port6_Configuration.Discrete2 Delay Mode
V_Port6_Configuration.Discrete2 Delay Timer 1 ms
V_Port6_Configuration.Discrete2 Delay Timer 2 ms
V_Port6_Configuration.Discrete2 Mirroring Enable
V_Port6_Configuration.Discrete2 Mirroring Port Selection
V_Port6_Configuration.Discrete2 Mirroring Channel Selection
V_Port6_Configuration.Discrete2 Mirroring Inversion
Port7 Configuration
V_Port7_Configuration.Discrete1 IO Selection
V_Port7_Configuration.Discrete1 Delay Mode
V_Port7_Configuration.Discrete1 Delay Timer 1 ms
V_Port7_Configuration.Discrete1 Delay Timer 2 ms
V_Port7_Configuration.Discrete1 Mirroring Enable
V_Port7_Configuration.Discrete1 Mirroring Port Selection
V_Port7_Configuration.Discrete1 Mirroring Channel Selection
V_Port7_Configuration.Discrete1 Mirroring Inversion
V_Port7_Configuration.Discrete2 IO Selection
V_Port7_Configuration.Discrete2 Delay Mode
V_Port7_Configuration.Discrete2 Delay Timer 1 ms
V_Port7_Configuration.Discrete2 Delay Timer 2 ms
V_Port7_Configuration.Discrete2 Mirroring Enable
V_Port7_Configuration.Discrete2 Mirroring Port Selection
V_Port7_Configuration.Discrete2 Mirroring Channel Selection
V_Port7_Configuration.Discrete2 Mirroring Inversion
Port8 Configuration
V_Port8_Configuration.Discrete1 IO Selection
V_Port8_Configuration.Discrete1 Delay Mode
V_Port8_Configuration.Discrete1 Delay Timer 1 ms
V_Port8_Configuration.Discrete1 Delay Timer 2 ms
V_Port8_Configuration.Discrete1 Mirroring Enable
V_Port8_Configuration.Discrete1 Mirroring Port Selection
V_Port8_Configuration.Discrete1 Mirroring Channel Selection
V_Port8_Configuration.Discrete1 Mirroring Inversion
V_Port8_Configuration.Discrete2 IO Selection
V_Port8_Configuration.Discrete2 Delay Mode
V_Port8_Configuration.Discrete2 Delay Timer 1 ms
V_Port8_Configuration.Discrete2 Delay Timer 2 ms
V_Port8_Configuration.Discrete2 Mirroring Enable
V_Port8_Configuration.Discrete2 Mirroring Port Selection
V_Port8_Configuration.Discrete2 Mirroring Channel Selection
V_Port8_Configuration.Discrete2 Mirroring Inversion
Discrete Host Out Mirroring Configuration
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Enable
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Port Selection
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Channel Selection
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Inversion
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Polarity
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Output Type
Process Data Grouping
V_Vendor_Specific_Configuration.Process Data Grouping

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
IO Metrics Ports 1 to 4
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Totalizer Counter
IO Metrics Ports 5 to 8
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Totalizer Counter

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

## Commissioning Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameters Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
Selectable Metric Reset
V_Selectable_Metric_Reset.Port1 Discrete1
V_Selectable_Metric_Reset.Port1 Discrete2
V_Selectable_Metric_Reset.Port2 Discrete1
V_Selectable_Metric_Reset.Port2 Discrete2
V_Selectable_Metric_Reset.Port3 Discrete1
V_Selectable_Metric_Reset.Port3 Discrete2
V_Selectable_Metric_Reset.Port4 Discrete1
V_Selectable_Metric_Reset.Port4 Discrete2
V_Selectable_Metric_Reset.Port5 Discrete1
V_Selectable_Metric_Reset.Port5 Discrete2
V_Selectable_Metric_Reset.Port6 Discrete1
V_Selectable_Metric_Reset.Port6 Discrete2
V_Selectable_Metric_Reset.Port7 Discrete1
V_Selectable_Metric_Reset.Port7 Discrete2
V_Selectable_Metric_Reset.Port8 Discrete1
V_Selectable_Metric_Reset.Port8 Discrete2
V_Selectable_Metric_Reset.Port1 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port1 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port2 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port2 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port3 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port3 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port4 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port4 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port5 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port5 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port6 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port6 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port7 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port7 Discrete2 Reset Count
V_Selectable_Metric_Reset.Port8 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port8 Discrete2 Reset Count
Access Locks
V_DeviceAccessLocks.Local Parameterization
V_DeviceAccessLocks.Local User Interface
Vendor Specific Configuration
Port1 Configuration
V_Port1_Configuration.Discrete1 IO Selection
V_Port1_Configuration.Discrete1 Delay Mode
V_Port1_Configuration.Discrete1 Delay Timer 1 ms
V_Port1_Configuration.Discrete1 Delay Timer 2 ms
V_Port1_Configuration.Discrete1 Mirroring Enable
V_Port1_Configuration.Discrete1 Mirroring Port Selection
V_Port1_Configuration.Discrete1 Mirroring Channel Selection
V_Port1_Configuration.Discrete1 Mirroring Inversion
V_Port1_Configuration.Discrete2 IO Selection
V_Port1_Configuration.Discrete2 Delay Mode
V_Port1_Configuration.Discrete2 Delay Timer 1 ms
V_Port1_Configuration.Discrete2 Delay Timer 2 ms
V_Port1_Configuration.Discrete2 Mirroring Enable
V_Port1_Configuration.Discrete2 Mirroring Port Selection
V_Port1_Configuration.Discrete2 Mirroring Channel Selection
V_Port1_Configuration.Discrete2 Mirroring Inversion
Port2 Configuration
V_Port2_Configuration.Discrete1 IO Selection
V_Port2_Configuration.Discrete1 Delay Mode
V_Port2_Configuration.Discrete1 Delay Timer 1 ms
V_Port2_Configuration.Discrete1 Delay Timer 2 ms
V_Port2_Configuration.Discrete1 Mirroring Enable
V_Port2_Configuration.Discrete1 Mirroring Port Selection
V_Port2_Configuration.Discrete1 Mirroring Channel Selection
V_Port2_Configuration.Discrete1 Mirroring Inversion
V_Port2_Configuration.Discrete2 IO Selection
V_Port2_Configuration.Discrete2 Delay Mode
V_Port2_Configuration.Discrete2 Delay Timer 1 ms
V_Port2_Configuration.Discrete2 Delay Timer 2 ms
V_Port2_Configuration.Discrete2 Mirroring Enable
V_Port2_Configuration.Discrete2 Mirroring Port Selection
V_Port2_Configuration.Discrete2 Mirroring Channel Selection
V_Port2_Configuration.Discrete2 Mirroring Inversion
Port3 Configuration
V_Port3_Configuration.Discrete1 IO Selection
V_Port3_Configuration.Discrete1 Delay Mode
V_Port3_Configuration.Discrete1 Delay Timer 1 ms
V_Port3_Configuration.Discrete1 Delay Timer 2 ms
V_Port3_Configuration.Discrete1 Mirroring Enable
V_Port3_Configuration.Discrete1 Mirroring Port Selection
V_Port3_Configuration.Discrete1 Mirroring Channel Selection
V_Port3_Configuration.Discrete1 Mirroring Inversion
V_Port3_Configuration.Discrete2 IO Selection
V_Port3_Configuration.Discrete2 Delay Mode
V_Port3_Configuration.Discrete2 Delay Timer 1 ms
V_Port3_Configuration.Discrete2 Delay Timer 2 ms
V_Port3_Configuration.Discrete2 Mirroring Enable
V_Port3_Configuration.Discrete2 Mirroring Port Selection
V_Port3_Configuration.Discrete2 Mirroring Channel Selection
V_Port3_Configuration.Discrete2 Mirroring Inversion
Port4 Configuration
V_Port4_Configuration.Discrete1 IO Selection
V_Port4_Configuration.Discrete1 Delay Mode
V_Port4_Configuration.Discrete1 Delay Timer 1 ms
V_Port4_Configuration.Discrete1 Delay Timer 2 ms
V_Port4_Configuration.Discrete1 Mirroring Enable
V_Port4_Configuration.Discrete1 Mirroring Port Selection
V_Port4_Configuration.Discrete1 Mirroring Channel Selection
V_Port4_Configuration.Discrete1 Mirroring Inversion
V_Port4_Configuration.Discrete2 IO Selection
V_Port4_Configuration.Discrete2 Delay Mode
V_Port4_Configuration.Discrete2 Delay Timer 1 ms
V_Port4_Configuration.Discrete2 Delay Timer 2 ms
V_Port4_Configuration.Discrete2 Mirroring Enable
V_Port4_Configuration.Discrete2 Mirroring Port Selection
V_Port4_Configuration.Discrete2 Mirroring Channel Selection
V_Port4_Configuration.Discrete2 Mirroring Inversion
Port5 Configuration
V_Port5_Configuration.Discrete1 IO Selection
V_Port5_Configuration.Discrete1 Delay Mode
V_Port5_Configuration.Discrete1 Delay Timer 1 ms
V_Port5_Configuration.Discrete1 Delay Timer 2 ms
V_Port5_Configuration.Discrete1 Mirroring Enable
V_Port5_Configuration.Discrete1 Mirroring Port Selection
V_Port5_Configuration.Discrete1 Mirroring Channel Selection
V_Port5_Configuration.Discrete1 Mirroring Inversion
V_Port5_Configuration.Discrete2 IO Selection
V_Port5_Configuration.Discrete2 Delay Mode
V_Port5_Configuration.Discrete2 Delay Timer 1 ms
V_Port5_Configuration.Discrete2 Delay Timer 2 ms
V_Port5_Configuration.Discrete2 Mirroring Enable
V_Port5_Configuration.Discrete2 Mirroring Port Selection
V_Port5_Configuration.Discrete2 Mirroring Channel Selection
V_Port5_Configuration.Discrete2 Mirroring Inversion
Port6 Configuration
V_Port6_Configuration.Discrete1 IO Selection
V_Port6_Configuration.Discrete1 Delay Mode
V_Port6_Configuration.Discrete1 Delay Timer 1 ms
V_Port6_Configuration.Discrete1 Delay Timer 2 ms
V_Port6_Configuration.Discrete1 Mirroring Enable
V_Port6_Configuration.Discrete1 Mirroring Port Selection
V_Port6_Configuration.Discrete1 Mirroring Channel Selection
V_Port6_Configuration.Discrete1 Mirroring Inversion
V_Port6_Configuration.Discrete2 IO Selection
V_Port6_Configuration.Discrete2 Delay Mode
V_Port6_Configuration.Discrete2 Delay Timer 1 ms
V_Port6_Configuration.Discrete2 Delay Timer 2 ms
V_Port6_Configuration.Discrete2 Mirroring Enable
V_Port6_Configuration.Discrete2 Mirroring Port Selection
V_Port6_Configuration.Discrete2 Mirroring Channel Selection
V_Port6_Configuration.Discrete2 Mirroring Inversion
Port7 Configuration
V_Port7_Configuration.Discrete1 IO Selection
V_Port7_Configuration.Discrete1 Delay Mode
V_Port7_Configuration.Discrete1 Delay Timer 1 ms
V_Port7_Configuration.Discrete1 Delay Timer 2 ms
V_Port7_Configuration.Discrete1 Mirroring Enable
V_Port7_Configuration.Discrete1 Mirroring Port Selection
V_Port7_Configuration.Discrete1 Mirroring Channel Selection
V_Port7_Configuration.Discrete1 Mirroring Inversion
V_Port7_Configuration.Discrete2 IO Selection
V_Port7_Configuration.Discrete2 Delay Mode
V_Port7_Configuration.Discrete2 Delay Timer 1 ms
V_Port7_Configuration.Discrete2 Delay Timer 2 ms
V_Port7_Configuration.Discrete2 Mirroring Enable
V_Port7_Configuration.Discrete2 Mirroring Port Selection
V_Port7_Configuration.Discrete2 Mirroring Channel Selection
V_Port7_Configuration.Discrete2 Mirroring Inversion
Port8 Configuration
V_Port8_Configuration.Discrete1 IO Selection
V_Port8_Configuration.Discrete1 Delay Mode
V_Port8_Configuration.Discrete1 Delay Timer 1 ms
V_Port8_Configuration.Discrete1 Delay Timer 2 ms
V_Port8_Configuration.Discrete1 Mirroring Enable
V_Port8_Configuration.Discrete1 Mirroring Port Selection
V_Port8_Configuration.Discrete1 Mirroring Channel Selection
V_Port8_Configuration.Discrete1 Mirroring Inversion
V_Port8_Configuration.Discrete2 IO Selection
V_Port8_Configuration.Discrete2 Delay Mode
V_Port8_Configuration.Discrete2 Delay Timer 1 ms
V_Port8_Configuration.Discrete2 Delay Timer 2 ms
V_Port8_Configuration.Discrete2 Mirroring Enable
V_Port8_Configuration.Discrete2 Mirroring Port Selection
V_Port8_Configuration.Discrete2 Mirroring Channel Selection
V_Port8_Configuration.Discrete2 Mirroring Inversion
Discrete Host Out Mirroring Configuration
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Enable
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Port Selection
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Channel Selection
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Inversion
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Polarity
V_Discrete_Host_Out_Mirroring_Configuration.Mirroring Output Type
Process Data Grouping
V_Vendor_Specific_Configuration.Process Data Grouping

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
IO Metrics Ports 1 to 4
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port1 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port1 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port2 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port2 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port3 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port3 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Count
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Duration µs
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port4 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Count
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Duration µs
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Events Per Minute
V_IO_Metrics_Ports_1_to_4.Port4 Discrete2 Totalizer Counter
IO Metrics Ports 5 to 8
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port5 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port5 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port6 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port6 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port7 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port7 Discrete2 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Count
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Duration µs
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port8 Discrete1 Totalizer Counter
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Count
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Duration µs
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Events Per Minute
V_IO_Metrics_Ports_5_to_8.Port8 Discrete2 Totalizer Counter

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.4.