Version: V1.0 | Release Date: 2024-11-01

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Menus]

IC70-16N-K
Vendor ID | 451 (0x01c3) |
Vendor Name | Banner Engineering Corporation
Vendor Text | More Sensors. More Solutions.
Vendor URL | www.bannerengineering.com/io-link
Device ID | 659480 (0x0a1018)
DeviceFamily | IC70-16N-K Series
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x4000 (Common Application Profile: Identification and Diagnosis)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: yes
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 3.3 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_0 with 1 octet on-request data OPERATE = TYPE_2_6 with 1 octet on-request data ISDU supported
Device Variant | IC70-16N-K
--- | ---
Description | NPN to IO-Link converter
Product ID | IC70-16N-K
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "Process Data Input" id=PD_ProcessDataIn

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 1 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
2 | 9 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 2 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
3 | 10 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 3 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
4 | 11 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 4 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
5 | 12 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 5 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
6 | 13 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 6 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
7 | 14 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 7 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
8 | 15 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 8 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
9 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 9 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
10 | 1 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 10 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
11 | 2 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 11 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
12 | 3 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 12 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
13 | 4 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 13 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
14 | 5 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 14 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
15 | 6 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 15 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input
16 | 7 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 16 Input State | true (1) = Channel Input Active. Note - even if is configured as an output, the active state will be reflected at the input

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

## ProcessDataOut "Process Data Output" id=PD_ProcessDataOut

bit length: 16
data type: 16-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 8 | Boolean | false = Off, true = On |  |  |  |  | Channel 1 Output State | true (1) = Channel Output Active
2 | 9 | Boolean | false = Off, true = On |  |  |  |  | Channel 2 Output State | true (1) = Channel Output Active
3 | 10 | Boolean | false = Off, true = On |  |  |  |  | Channel 3 Output State | true (1) = Channel Output Active
4 | 11 | Boolean | false = Off, true = On |  |  |  |  | Channel 4 Output State | true (1) = Channel Output Active
5 | 12 | Boolean | false = Off, true = On |  |  |  |  | Channel 5 Output State | true (1) = Channel Output Active
6 | 13 | Boolean | false = Off, true = On |  |  |  |  | Channel 6 Output State | true (1) = Channel Output Active
7 | 14 | Boolean | false = Off, true = On |  |  |  |  | Channel 7 Output State | true (1) = Channel Output Active
8 | 15 | Boolean | false = Off, true = On |  |  |  |  | Channel 8 Output State | true (1) = Channel Output Active
9 | 0 | Boolean | false = Off, true = On |  |  |  |  | Channel 9 Output State | true (1) = Channel Output Active
10 | 1 | Boolean | false = Off, true = On |  |  |  |  | Channel 10 Output State | true (1) = Channel Output Active
11 | 2 | Boolean | false = Off, true = On |  |  |  |  | Channel 11 Output State | true (1) = Channel Output Active
12 | 3 | Boolean | false = Off, true = On |  |  |  |  | Channel 12 Output State | true (1) = Channel Output Active
13 | 4 | Boolean | false = Off, true = On |  |  |  |  | Channel 13 Output State | true (1) = Channel Output Active
14 | 5 | Boolean | false = Off, true = On |  |  |  |  | Channel 14 Output State | true (1) = Channel Output Active
15 | 6 | Boolean | false = Off, true = On |  |  |  |  | Channel 15 Output State | true (1) = Channel Output Active
16 | 7 | Boolean | false = Off, true = On |  |  |  |  | Channel 16 Output State | true (1) = Channel Output Active

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

[Top]

## Standard Variable "Direct Parameters - Page 1" index=0 id=V_DirectParameters_1

description: Comprises the required parameters defining the communication characteristics and identifiers for device validation.
data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time | Communication: Current communication cycle duration used by the master. This value defines the process data cycle.
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time | Communication: Minimum communication cycle duration supported by the device. This value defines the lowest possible process data cycle.
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability | Communication: Information on the structure and the supported features of the communication messages.
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Revision ID | Communication: Identifier for the currently used communication protocol revision.
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length | Communication: Information on width and features of the process input data (Process Data from Device to Master).
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length | Communication: Information on width of the process output data (Process Data from Master to Device).
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 | Identification: Highest octet of the Vendor ID. Combined with the parameter Vendor ID 2, this parameter defines the 16-bit value of the unique Vendor ID as assigned by the IO-Link Community.
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 | Identification: Lowest octet of the Vendor ID. Combined with the parameter Vendor ID 1, this parameter defines the 16-bit value of the unique Vendor ID as assigned by the IO-Link Community.
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 | Identification: Highest octet of the Device ID. Combined with the parameters Device ID 2 and 3, this parameter defines the 24-bit value of the vendor-specific Device ID.
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 | Identification: Middle octet of the Device ID. Combined with the parameters Device ID 1 and 3, this parameter defines the 24-bit value of the vendor-specific Device ID.
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 | Identification: Lowest octet of the Device ID. Combined with the parameters Device ID 1 and 2, this parameter defines the 24-bit value of the vendor-specific Device ID.
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger |  |  | wo | X |  | System Command | Application: Command interface for devices without ISDU support. Validity and execution of commands are not confirmed.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters - Page 2" index=1 id=V_DirectParameters_2

description: A set of parameters for devices without ISDU support.
data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device-specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "System Command" index=2 id=V_SystemCommand

description: Command interface for applications. A positive acknowledge indicates the complete and correct finalization of the requested function.
data type: 8-bit UInteger
allowed values: 130 = Restore Factory Settings, 162 = Discovery Start, 163 = Discovery Stop, 164 = Reset All Metrics
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

description: The access to the device parameters can be restricted by setting appropriate flags within this parameter.
data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Parameter Write Access | This lock prevents the write access to all read/write parameters of the device except for the parameter 'Device Access Locks'.
2 | 1 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Data Storage | This lock prevents the write access to the device parameters via the data storage mechanism.
3 | 2 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Local Parameterization | This lock prevents the device settings from being changed via local operating elements on the device.
4 | 3 | Boolean | false = Unlocked, true = Locked |  |  |  |  | Local User Interface | This lock prevents the access to the device settings and display via a local user interface. The user interface is disabled.

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

description: The vendor name that is assigned to a Vendor ID.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

description: Additional information about the vendor.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

description: Complete product name.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

description: Vendor-specific product or type identification (e.g., item number or model number).
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

description: Additional product information for the device.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

description: Unique, vendor-specific identifier of the individual device.
data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Revision" index=23 id=V_FirmwareRevision

description: Unique, vendor-specific identifier of the firmware revision of the individual device.
data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application-specific Tag" index=24 id=V_ApplicationSpecificTag

description: Possibility to mark a device with user- or application-specific information.
data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

description: Indicator for the current device condition and diagnosis state.
data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

description: List of all currently pending events in the device.
data type: Array[6] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 6 | 6 |

## Standard Variable "PD Input" index=40 id=V_ProcessDataInput

description: Last valid process input data of the device.
data type: see ProcessDataIn!
access rights: ro
dynamic

## Standard Variable "PD Output" index=41 id=V_ProcessDataOutput

description: Last valid process output data written to the device.
data type: see ProcessDataOut!
access rights: ro
dynamic
[Top]

## Variable "All-time Run Time" index=69 id=V_AllTimeRunTime

description: A read only run time counter (in hours) that tracks the total time the sensor has been running since manufacture
data type: 32-bit Record (subindex access not supported)
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time" index=70 id=V_ResetableRunTime

description: A read / write run time counter (in hours) that can be monitored or set by the user
data type: 32-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "All-time Run Time Event Time" index=78 id=V_AllTimeRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Event indicating the corresponding configured running time has elapsed.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time Event Time" index=79 id=V_ResetableRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "IO Metrics Channels 1 to 8" index=80 id=V_IO_Metrics_Channel_1_to_8

description: IO Metrics Channels 1 to 8
data type: 1024-bit Record
access rights: ro
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer |  |  |  |  |  | Channel1 Count |
2 | 32 | 32-bit Integer |  |  |  |  |  | Channel1 Duration |
3 | 64 | 32-bit Integer |  |  |  |  |  | Channel1 Events Per Minute |
4 | 96 | 32-bit Integer |  |  |  |  |  | Channel1 Totalizer Counter |
5 | 128 | 32-bit Integer |  |  |  |  |  | Channel2 Count |
6 | 160 | 32-bit Integer |  |  |  |  |  | Channel2 Duration |
7 | 192 | 32-bit Integer |  |  |  |  |  | Channel2 Events Per Minute |
8 | 224 | 32-bit Integer |  |  |  |  |  | Channel2 Totalizer Counter |
9 | 256 | 32-bit Integer |  |  |  |  |  | Channel3 Count |
10 | 288 | 32-bit Integer |  |  |  |  |  | Channel3 Duration |
11 | 320 | 32-bit Integer |  |  |  |  |  | Channel3 Events Per Minute |
12 | 352 | 32-bit Integer |  |  |  |  |  | Channel3 Totalizer Counter |
13 | 384 | 32-bit Integer |  |  |  |  |  | Channel4 Count |
14 | 416 | 32-bit Integer |  |  |  |  |  | Channel4 Duration |
15 | 448 | 32-bit Integer |  |  |  |  |  | Channel4 Events Per Minute |
16 | 480 | 32-bit Integer |  |  |  |  |  | Channel4 Totalizer Counter |
17 | 512 | 32-bit Integer |  |  |  |  |  | Channel5 Count |
18 | 544 | 32-bit Integer |  |  |  |  |  | Channel5 Duration |
19 | 576 | 32-bit Integer |  |  |  |  |  | Channel5 Events Per Minute |
20 | 608 | 32-bit Integer |  |  |  |  |  | Channel5 Totalizer Counter |
21 | 640 | 32-bit Integer |  |  |  |  |  | Channel6 Count |
22 | 672 | 32-bit Integer |  |  |  |  |  | Channel6 Duration |
23 | 704 | 32-bit Integer |  |  |  |  |  | Channel6 Events Per Minute |
24 | 736 | 32-bit Integer |  |  |  |  |  | Channel6 Totalizer Counter |
25 | 768 | 32-bit Integer |  |  |  |  |  | Channel7 Count |
26 | 800 | 32-bit Integer |  |  |  |  |  | Channel7 Duration |
27 | 832 | 32-bit Integer |  |  |  |  |  | Channel7 Events Per Minute |
28 | 864 | 32-bit Integer |  |  |  |  |  | Channel7 Totalizer Counter |
29 | 896 | 32-bit Integer |  |  |  |  |  | Channel8 Count |
30 | 928 | 32-bit Integer |  |  |  |  |  | Channel8 Duration |
31 | 960 | 32-bit Integer |  |  |  |  |  | Channel8 Events Per Minute |
32 | 992 | 32-bit Integer |  |  |  |  |  | Channel8 Totalizer Counter |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 1023 - 1016 | 1015 - 1008 | 1007 - 1000 | 999 - 992 | 991 - 984 | 983 - 976 | 975 - 968 | 967 - 960
subindex | 32 | 32 | 32 | 32 | 31 | 31 | 31 | 31
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 959 - 952 | 951 - 944 | 943 - 936 | 935 - 928 | 927 - 920 | 919 - 912 | 911 - 904 | 903 - 896
subindex | 30 | 30 | 30 | 30 | 29 | 29 | 29 | 29
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 895 - 888 | 887 - 880 | 879 - 872 | 871 - 864 | 863 - 856 | 855 - 848 | 847 - 840 | 839 - 832
subindex | 28 | 28 | 28 | 28 | 27 | 27 | 27 | 27
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 831 - 824 | 823 - 816 | 815 - 808 | 807 - 800 | 799 - 792 | 791 - 784 | 783 - 776 | 775 - 768
subindex | 26 | 26 | 26 | 26 | 25 | 25 | 25 | 25
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 767 - 760 | 759 - 752 | 751 - 744 | 743 - 736 | 735 - 728 | 727 - 720 | 719 - 712 | 711 - 704
subindex | 24 | 24 | 24 | 24 | 23 | 23 | 23 | 23
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 703 - 696 | 695 - 688 | 687 - 680 | 679 - 672 | 671 - 664 | 663 - 656 | 655 - 648 | 647 - 640
subindex | 22 | 22 | 22 | 22 | 21 | 21 | 21 | 21
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 639 - 632 | 631 - 624 | 623 - 616 | 615 - 608 | 607 - 600 | 599 - 592 | 591 - 584 | 583 - 576
subindex | 20 | 20 | 20 | 20 | 19 | 19 | 19 | 19
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 575 - 568 | 567 - 560 | 559 - 552 | 551 - 544 | 543 - 536 | 535 - 528 | 527 - 520 | 519 - 512
subindex | 18 | 18 | 18 | 18 | 17 | 17 | 17 | 17
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 64 | 65 | 66 | 67 | 68 | 69 | 70 | 71
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448
subindex | 16 | 16 | 16 | 16 | 15 | 15 | 15 | 15
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 72 | 73 | 74 | 75 | 76 | 77 | 78 | 79
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384
subindex | 14 | 14 | 14 | 14 | 13 | 13 | 13 | 13
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 80 | 81 | 82 | 83 | 84 | 85 | 86 | 87
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320
subindex | 12 | 12 | 12 | 12 | 11 | 11 | 11 | 11
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 88 | 89 | 90 | 91 | 92 | 93 | 94 | 95
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256
subindex | 10 | 10 | 10 | 10 | 9 | 9 | 9 | 9
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 96 | 97 | 98 | 99 | 100 | 101 | 102 | 103
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192
subindex | 8 | 8 | 8 | 8 | 7 | 7 | 7 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 104 | 105 | 106 | 107 | 108 | 109 | 110 | 111
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128
subindex | 6 | 6 | 6 | 6 | 5 | 5 | 5 | 5
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 112 | 113 | 114 | 115 | 116 | 117 | 118 | 119
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 4 | 4 | 4 | 4 | 3 | 3 | 3 | 3
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 120 | 121 | 122 | 123 | 124 | 125 | 126 | 127
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 1
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "IO Metrics Channels 9 to 16" index=81 id=V_IO_Metrics_Channel_9_to_16

description: IO Metrics Channels 9 to 16 Values
data type: 1024-bit Record
access rights: ro
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer |  |  |  |  |  | Channel9 Count |
2 | 32 | 32-bit Integer |  |  |  |  |  | Channel9 Duration |
3 | 64 | 32-bit Integer |  |  |  |  |  | Channel9 Events Per Minute |
4 | 96 | 32-bit Integer |  |  |  |  |  | Channel9 Totalizer Counter |
5 | 128 | 32-bit Integer |  |  |  |  |  | Channel10 Count |
6 | 160 | 32-bit Integer |  |  |  |  |  | Channel10 Duration |
7 | 192 | 32-bit Integer |  |  |  |  |  | Channel10 Events Per Minute |
8 | 224 | 32-bit Integer |  |  |  |  |  | Channel10 Totalizer Counter |
9 | 256 | 32-bit Integer |  |  |  |  |  | Channel11 Count |
10 | 288 | 32-bit Integer |  |  |  |  |  | Channel11 Duration |
11 | 320 | 32-bit Integer |  |  |  |  |  | Channel11 Events Per Minute |
12 | 352 | 32-bit Integer |  |  |  |  |  | Channel11 Totalizer Counter |
13 | 384 | 32-bit Integer |  |  |  |  |  | Channel12 Count |
14 | 416 | 32-bit Integer |  |  |  |  |  | Channel12 Duration |
15 | 448 | 32-bit Integer |  |  |  |  |  | Channel12 Events Per Minute |
16 | 480 | 32-bit Integer |  |  |  |  |  | Channel12 Totalizer Counter |
17 | 512 | 32-bit Integer |  |  |  |  |  | Channel13 Count |
18 | 544 | 32-bit Integer |  |  |  |  |  | Channel13 Duration |
19 | 576 | 32-bit Integer |  |  |  |  |  | Channel13 Events Per Minute |
20 | 608 | 32-bit Integer |  |  |  |  |  | Channel13 Totalizer Counter |
21 | 640 | 32-bit Integer |  |  |  |  |  | Channel14 Count |
22 | 672 | 32-bit Integer |  |  |  |  |  | Channel14 Duration |
23 | 704 | 32-bit Integer |  |  |  |  |  | Channel14 Events Per Minute |
24 | 736 | 32-bit Integer |  |  |  |  |  | Channel14 Totalizer Counter |
25 | 768 | 32-bit Integer |  |  |  |  |  | Channel15 Count |
26 | 800 | 32-bit Integer |  |  |  |  |  | Channel15 Duration |
27 | 832 | 32-bit Integer |  |  |  |  |  | Channel15 Events Per Minute |
28 | 864 | 32-bit Integer |  |  |  |  |  | Channel15 Totalizer Counter |
29 | 896 | 32-bit Integer |  |  |  |  |  | Channel16 Count |
30 | 928 | 32-bit Integer |  |  |  |  |  | Channel16 Duration |
31 | 960 | 32-bit Integer |  |  |  |  |  | Channel16 Events Per Minute |
32 | 992 | 32-bit Integer |  |  |  |  |  | Channel16 Totalizer Counter |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 1023 - 1016 | 1015 - 1008 | 1007 - 1000 | 999 - 992 | 991 - 984 | 983 - 976 | 975 - 968 | 967 - 960
subindex | 32 | 32 | 32 | 32 | 31 | 31 | 31 | 31
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 959 - 952 | 951 - 944 | 943 - 936 | 935 - 928 | 927 - 920 | 919 - 912 | 911 - 904 | 903 - 896
subindex | 30 | 30 | 30 | 30 | 29 | 29 | 29 | 29
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 895 - 888 | 887 - 880 | 879 - 872 | 871 - 864 | 863 - 856 | 855 - 848 | 847 - 840 | 839 - 832
subindex | 28 | 28 | 28 | 28 | 27 | 27 | 27 | 27
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 831 - 824 | 823 - 816 | 815 - 808 | 807 - 800 | 799 - 792 | 791 - 784 | 783 - 776 | 775 - 768
subindex | 26 | 26 | 26 | 26 | 25 | 25 | 25 | 25
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 767 - 760 | 759 - 752 | 751 - 744 | 743 - 736 | 735 - 728 | 727 - 720 | 719 - 712 | 711 - 704
subindex | 24 | 24 | 24 | 24 | 23 | 23 | 23 | 23
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 703 - 696 | 695 - 688 | 687 - 680 | 679 - 672 | 671 - 664 | 663 - 656 | 655 - 648 | 647 - 640
subindex | 22 | 22 | 22 | 22 | 21 | 21 | 21 | 21
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 639 - 632 | 631 - 624 | 623 - 616 | 615 - 608 | 607 - 600 | 599 - 592 | 591 - 584 | 583 - 576
subindex | 20 | 20 | 20 | 20 | 19 | 19 | 19 | 19
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 575 - 568 | 567 - 560 | 559 - 552 | 551 - 544 | 543 - 536 | 535 - 528 | 527 - 520 | 519 - 512
subindex | 18 | 18 | 18 | 18 | 17 | 17 | 17 | 17
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 64 | 65 | 66 | 67 | 68 | 69 | 70 | 71
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448
subindex | 16 | 16 | 16 | 16 | 15 | 15 | 15 | 15
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 72 | 73 | 74 | 75 | 76 | 77 | 78 | 79
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384
subindex | 14 | 14 | 14 | 14 | 13 | 13 | 13 | 13
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 80 | 81 | 82 | 83 | 84 | 85 | 86 | 87
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320
subindex | 12 | 12 | 12 | 12 | 11 | 11 | 11 | 11
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 88 | 89 | 90 | 91 | 92 | 93 | 94 | 95
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256
subindex | 10 | 10 | 10 | 10 | 9 | 9 | 9 | 9
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 96 | 97 | 98 | 99 | 100 | 101 | 102 | 103
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192
subindex | 8 | 8 | 8 | 8 | 7 | 7 | 7 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 104 | 105 | 106 | 107 | 108 | 109 | 110 | 111
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128
subindex | 6 | 6 | 6 | 6 | 5 | 5 | 5 | 5
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 112 | 113 | 114 | 115 | 116 | 117 | 118 | 119
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 4 | 4 | 4 | 4 | 3 | 3 | 3 | 3
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 120 | 121 | 122 | 123 | 124 | 125 | 126 | 127
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 1
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Selectable Metric Reset" index=82 id=V_Selectable_Metric_Reset

description: User can select which channel / Channels to reset
data type: 528-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel1 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
2 | 1 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel2 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
3 | 2 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel3 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
4 | 3 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel4 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
5 | 4 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel5 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
6 | 5 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel6 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
7 | 6 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel7 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
8 | 7 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel8 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
9 | 8 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel9 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
10 | 9 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel10 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
11 | 10 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel11 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
12 | 11 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel12 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
13 | 12 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel13 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
14 | 13 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel14 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
15 | 14 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel15 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
16 | 15 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Channel16 | If set to [Reset], Channel metrics will be reset. Note - the Count value can be set to a non-zero value using [Channel# Reset Count]
17 | 16 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel1 Reset Count |
18 | 48 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel2 Reset Count |
19 | 80 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel3 Reset Count |
20 | 112 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel4 Reset Count |
21 | 144 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel5 Reset Count |
22 | 176 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel6 Reset Count |
23 | 208 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel7 Reset Count |
24 | 240 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel8 Reset Count |
25 | 272 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel9 Reset Count |
26 | 304 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel10 Reset Count |
27 | 336 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel11 Reset Count |
28 | 368 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel12 Reset Count |
29 | 400 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel13 Reset Count |
30 | 432 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel14 Reset Count |
31 | 464 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel15 Reset Count |
32 | 496 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Channel16 Reset Count |

Octet 0

bit offset | 527 | 526 | 525 | 524 | 523 | 522 | 521 | 520
subindex | 32
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 1

bit offset | 519 | 518 | 517 | 516 | 515 | 514 | 513 | 512
subindex | 32
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 2

bit offset | 511 | 510 | 509 | 508 | 507 | 506 | 505 | 504
subindex | 32
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 3

bit offset | 503 | 502 | 501 | 500 | 499 | 498 | 497 | 496
subindex | 32
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 495 | 494 | 493 | 492 | 491 | 490 | 489 | 488
subindex | 31
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 5

bit offset | 487 | 486 | 485 | 484 | 483 | 482 | 481 | 480
subindex | 31
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 6

bit offset | 479 | 478 | 477 | 476 | 475 | 474 | 473 | 472
subindex | 31
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 7

bit offset | 471 | 470 | 469 | 468 | 467 | 466 | 465 | 464
subindex | 31
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 8

bit offset | 463 | 462 | 461 | 460 | 459 | 458 | 457 | 456
subindex | 30
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 9

bit offset | 455 | 454 | 453 | 452 | 451 | 450 | 449 | 448
subindex | 30
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 10

bit offset | 447 | 446 | 445 | 444 | 443 | 442 | 441 | 440
subindex | 30
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 11

bit offset | 439 | 438 | 437 | 436 | 435 | 434 | 433 | 432
subindex | 30
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 12

bit offset | 431 | 430 | 429 | 428 | 427 | 426 | 425 | 424
subindex | 29
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 13

bit offset | 423 | 422 | 421 | 420 | 419 | 418 | 417 | 416
subindex | 29
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 14

bit offset | 415 | 414 | 413 | 412 | 411 | 410 | 409 | 408
subindex | 29
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 15

bit offset | 407 | 406 | 405 | 404 | 403 | 402 | 401 | 400
subindex | 29
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 16

bit offset | 399 | 398 | 397 | 396 | 395 | 394 | 393 | 392
subindex | 28
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 17

bit offset | 391 | 390 | 389 | 388 | 387 | 386 | 385 | 384
subindex | 28
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 18

bit offset | 383 | 382 | 381 | 380 | 379 | 378 | 377 | 376
subindex | 28
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 19

bit offset | 375 | 374 | 373 | 372 | 371 | 370 | 369 | 368
subindex | 28
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 20

bit offset | 367 | 366 | 365 | 364 | 363 | 362 | 361 | 360
subindex | 27
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 21

bit offset | 359 | 358 | 357 | 356 | 355 | 354 | 353 | 352
subindex | 27
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 22

bit offset | 351 | 350 | 349 | 348 | 347 | 346 | 345 | 344
subindex | 27
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 23

bit offset | 343 | 342 | 341 | 340 | 339 | 338 | 337 | 336
subindex | 27
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 24

bit offset | 335 | 334 | 333 | 332 | 331 | 330 | 329 | 328
subindex | 26
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 25

bit offset | 327 | 326 | 325 | 324 | 323 | 322 | 321 | 320
subindex | 26
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 26

bit offset | 319 | 318 | 317 | 316 | 315 | 314 | 313 | 312
subindex | 26
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 27

bit offset | 311 | 310 | 309 | 308 | 307 | 306 | 305 | 304
subindex | 26
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 28

bit offset | 303 | 302 | 301 | 300 | 299 | 298 | 297 | 296
subindex | 25
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 29

bit offset | 295 | 294 | 293 | 292 | 291 | 290 | 289 | 288
subindex | 25
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 30

bit offset | 287 | 286 | 285 | 284 | 283 | 282 | 281 | 280
subindex | 25
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 31

bit offset | 279 | 278 | 277 | 276 | 275 | 274 | 273 | 272
subindex | 25
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 32

bit offset | 271 | 270 | 269 | 268 | 267 | 266 | 265 | 264
subindex | 24
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 33

bit offset | 263 | 262 | 261 | 260 | 259 | 258 | 257 | 256
subindex | 24
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 34

bit offset | 255 | 254 | 253 | 252 | 251 | 250 | 249 | 248
subindex | 24
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 35

bit offset | 247 | 246 | 245 | 244 | 243 | 242 | 241 | 240
subindex | 24
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 36

bit offset | 239 | 238 | 237 | 236 | 235 | 234 | 233 | 232
subindex | 23
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 37

bit offset | 231 | 230 | 229 | 228 | 227 | 226 | 225 | 224
subindex | 23
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 38

bit offset | 223 | 222 | 221 | 220 | 219 | 218 | 217 | 216
subindex | 23
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 39

bit offset | 215 | 214 | 213 | 212 | 211 | 210 | 209 | 208
subindex | 23
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 40

bit offset | 207 | 206 | 205 | 204 | 203 | 202 | 201 | 200
subindex | 22
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 41

bit offset | 199 | 198 | 197 | 196 | 195 | 194 | 193 | 192
subindex | 22
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 42

bit offset | 191 | 190 | 189 | 188 | 187 | 186 | 185 | 184
subindex | 22
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 43

bit offset | 183 | 182 | 181 | 180 | 179 | 178 | 177 | 176
subindex | 22
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 44

bit offset | 175 | 174 | 173 | 172 | 171 | 170 | 169 | 168
subindex | 21
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 45

bit offset | 167 | 166 | 165 | 164 | 163 | 162 | 161 | 160
subindex | 21
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 46

bit offset | 159 | 158 | 157 | 156 | 155 | 154 | 153 | 152
subindex | 21
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 47

bit offset | 151 | 150 | 149 | 148 | 147 | 146 | 145 | 144
subindex | 21
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 48

bit offset | 143 | 142 | 141 | 140 | 139 | 138 | 137 | 136
subindex | 20
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 49

bit offset | 135 | 134 | 133 | 132 | 131 | 130 | 129 | 128
subindex | 20
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 50

bit offset | 127 | 126 | 125 | 124 | 123 | 122 | 121 | 120
subindex | 20
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 51

bit offset | 119 | 118 | 117 | 116 | 115 | 114 | 113 | 112
subindex | 20
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 52

bit offset | 111 | 110 | 109 | 108 | 107 | 106 | 105 | 104
subindex | 19
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 53

bit offset | 103 | 102 | 101 | 100 | 99 | 98 | 97 | 96
subindex | 19
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 54

bit offset | 95 | 94 | 93 | 92 | 91 | 90 | 89 | 88
subindex | 19
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 55

bit offset | 87 | 86 | 85 | 84 | 83 | 82 | 81 | 80
subindex | 19
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 56

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | 18
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 57

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | 18
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 58

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 18
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 59

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 18
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 60

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | 17
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 61

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 17
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 62

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 17
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 63

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 17
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 64

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 16 | 15 | 14 | 13 | 12 | 11 | 10 | 9

Octet 65

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1

## Variable "Channel1 Configuration" index=87 id=V_channel1_Configuration

description: Channel1 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel2 Configuration" index=88 id=V_channel2_Configuration

description: Channel2 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel3 Configuration" index=89 id=V_channel3_Configuration

description: Channel3 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel4 Configuration" index=90 id=V_channel4_Configuration

description: Channel4 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel5 Configuration" index=91 id=V_channel5_Configuration

description: Channel5 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel6 Configuration" index=92 id=V_channel6_Configuration

description: Channel6 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel7 Configuration" index=93 id=V_channel7_Configuration

description: Channel7 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel8 Configuration" index=94 id=V_channel8_Configuration

description: Channel8 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel9 Configuration" index=95 id=V_channel9_Configuration

description: Channel9 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel10 Configuration" index=96 id=V_channel10_Configuration

description: Channel10 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel11 Configuration" index=97 id=V_channel11_Configuration

description: Channel11 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel12 Configuration" index=98 id=V_channel12_Configuration

description: Channel12 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel13 Configuration" index=99 id=V_channel13_Configuration

description: Channel13 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel14 Configuration" index=100 id=V_channel14_Configuration

description: Channel14 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel15 Configuration" index=101 id=V_channel15_Configuration

description: Channel15 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Channel16 Configuration" index=102 id=V_channel16_Configuration

description: Channel16 Configuration
data type: 104-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 2 = NPN Output with Pull Up | 2 |  |  |  | IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Delay Mode | Channel Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 1 | Channel On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Delay Timer 2 | Channel Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
6 | 88 | 8-bit UInteger | 0 = Channel 1, 1 = Channel 2, 2 = Channel 3, 3 = Channel 4, 4 = Channel 5, 5 = Channel 6, 6 = Channel 7, 7 = Channel 8, 8 = Channel 9, 9 = Channel 10, 10 = Channel 11, 11 = Channel 12, 12 = Channel 13, 13 = Channel 14, 14 = Channel 15, 15 = Channel 16 | 0 |  |  |  | Mirroring Channel Selection |
7 | 96 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40
subindex | 7 | 6 | 5 | 4 | 4 | 4 | 4 | 3
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24

octet | 8 | 9 | 10 | 11 | 12 |
bit offset | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 3 | 2 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
25376 (0x6320) | Error | Parameter error | Check datasheet and values
36000 (0x8ca0) | Warning | All-time Run Time Event | Event indicating the corresponding configured running time has elapsed.
36001 (0x8ca1) | Warning | Resetable Run Time Event | Event indicating the corresponding configured running time has elapsed.

[Top]

## Operator Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_ApplicationSpecificTag

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
IO Metrics Channels 1 to 8
V_IO_Metrics_Channel_1_to_8.Channel1 Count
V_IO_Metrics_Channel_1_to_8.Channel1 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel1 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel1 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel2 Count
V_IO_Metrics_Channel_1_to_8.Channel2 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel2 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel2 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel3 Count
V_IO_Metrics_Channel_1_to_8.Channel3 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel3 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel3 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel4 Count
V_IO_Metrics_Channel_1_to_8.Channel4 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel4 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel4 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel5 Count
V_IO_Metrics_Channel_1_to_8.Channel5 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel5 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel5 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel6 Count
V_IO_Metrics_Channel_1_to_8.Channel6 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel6 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel6 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel7 Count
V_IO_Metrics_Channel_1_to_8.Channel7 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel7 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel7 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel8 Count
V_IO_Metrics_Channel_1_to_8.Channel8 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel8 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel8 Totalizer Counter
IO Metrics Channels 9 to 16
V_IO_Metrics_Channel_9_to_16.Channel9 Count
V_IO_Metrics_Channel_9_to_16.Channel9 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel9 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel9 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel10 Count
V_IO_Metrics_Channel_9_to_16.Channel10 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel10 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel10 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel11 Count
V_IO_Metrics_Channel_9_to_16.Channel11 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel11 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel11 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel12 Count
V_IO_Metrics_Channel_9_to_16.Channel12 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel12 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel12 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel13 Count
V_IO_Metrics_Channel_9_to_16.Channel13 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel13 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel13 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel14 Count
V_IO_Metrics_Channel_9_to_16.Channel14 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel14 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel14 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel15 Count
V_IO_Metrics_Channel_9_to_16.Channel15 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel15 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel15 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel16 Count
V_IO_Metrics_Channel_9_to_16.Channel16 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel16 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel16 Totalizer Counter

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameters Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
Selectable Metric Reset
V_Selectable_Metric_Reset.Channel1
V_Selectable_Metric_Reset.Channel2
V_Selectable_Metric_Reset.Channel3
V_Selectable_Metric_Reset.Channel4
V_Selectable_Metric_Reset.Channel5
V_Selectable_Metric_Reset.Channel6
V_Selectable_Metric_Reset.Channel7
V_Selectable_Metric_Reset.Channel8
V_Selectable_Metric_Reset.Channel9
V_Selectable_Metric_Reset.Channel10
V_Selectable_Metric_Reset.Channel11
V_Selectable_Metric_Reset.Channel12
V_Selectable_Metric_Reset.Channel13
V_Selectable_Metric_Reset.Channel14
V_Selectable_Metric_Reset.Channel15
V_Selectable_Metric_Reset.Channel16
V_Selectable_Metric_Reset.Channel1 Reset Count
V_Selectable_Metric_Reset.Channel2 Reset Count
V_Selectable_Metric_Reset.Channel3 Reset Count
V_Selectable_Metric_Reset.Channel4 Reset Count
V_Selectable_Metric_Reset.Channel5 Reset Count
V_Selectable_Metric_Reset.Channel6 Reset Count
V_Selectable_Metric_Reset.Channel7 Reset Count
V_Selectable_Metric_Reset.Channel8 Reset Count
V_Selectable_Metric_Reset.Channel9 Reset Count
V_Selectable_Metric_Reset.Channel10 Reset Count
V_Selectable_Metric_Reset.Channel11 Reset Count
V_Selectable_Metric_Reset.Channel12 Reset Count
V_Selectable_Metric_Reset.Channel13 Reset Count
V_Selectable_Metric_Reset.Channel14 Reset Count
V_Selectable_Metric_Reset.Channel15 Reset Count
V_Selectable_Metric_Reset.Channel16 Reset Count
Access Locks
V_DeviceAccessLocks.Local Parameterization
V_DeviceAccessLocks.Local User Interface
Vendor Specific Configuration
Channel1 Configuration
V_channel1_Configuration.IO Selection
V_channel1_Configuration.Delay Mode
V_channel1_Configuration.Delay Timer 1 ms
V_channel1_Configuration.Delay Timer 2 ms
V_channel1_Configuration.Mirroring Enable
V_channel1_Configuration.Mirroring Channel Selection
V_channel1_Configuration.Mirroring Inversion
Channel2 Configuration
V_channel2_Configuration.IO Selection
V_channel2_Configuration.Delay Mode
V_channel2_Configuration.Delay Timer 1 ms
V_channel2_Configuration.Delay Timer 2 ms
V_channel2_Configuration.Mirroring Enable
V_channel2_Configuration.Mirroring Channel Selection
V_channel2_Configuration.Mirroring Inversion
Channel3 Configuration
V_channel3_Configuration.IO Selection
V_channel3_Configuration.Delay Mode
V_channel3_Configuration.Delay Timer 1 ms
V_channel3_Configuration.Delay Timer 2 ms
V_channel3_Configuration.Mirroring Enable
V_channel3_Configuration.Mirroring Channel Selection
V_channel3_Configuration.Mirroring Inversion
Channel4 Configuration
V_channel4_Configuration.IO Selection
V_channel4_Configuration.Delay Mode
V_channel4_Configuration.Delay Timer 1 ms
V_channel4_Configuration.Delay Timer 2 ms
V_channel4_Configuration.Mirroring Enable
V_channel4_Configuration.Mirroring Channel Selection
V_channel4_Configuration.Mirroring Inversion
Channel5 Configuration
V_channel5_Configuration.IO Selection
V_channel5_Configuration.Delay Mode
V_channel5_Configuration.Delay Timer 1 ms
V_channel5_Configuration.Delay Timer 2 ms
V_channel5_Configuration.Mirroring Enable
V_channel5_Configuration.Mirroring Channel Selection
V_channel5_Configuration.Mirroring Inversion
Channel6 Configuration
V_channel6_Configuration.IO Selection
V_channel6_Configuration.Delay Mode
V_channel6_Configuration.Delay Timer 1 ms
V_channel6_Configuration.Delay Timer 2 ms
V_channel6_Configuration.Mirroring Enable
V_channel6_Configuration.Mirroring Channel Selection
V_channel6_Configuration.Mirroring Inversion
Channel7 Configuration
V_channel7_Configuration.IO Selection
V_channel7_Configuration.Delay Mode
V_channel7_Configuration.Delay Timer 1 ms
V_channel7_Configuration.Delay Timer 2 ms
V_channel7_Configuration.Mirroring Enable
V_channel7_Configuration.Mirroring Channel Selection
V_channel7_Configuration.Mirroring Inversion
Channel8 Configuration
V_channel8_Configuration.IO Selection
V_channel8_Configuration.Delay Mode
V_channel8_Configuration.Delay Timer 1 ms
V_channel8_Configuration.Delay Timer 2 ms
V_channel8_Configuration.Mirroring Enable
V_channel8_Configuration.Mirroring Channel Selection
V_channel8_Configuration.Mirroring Inversion
Channel9 Configuration
V_channel9_Configuration.IO Selection
V_channel9_Configuration.Delay Mode
V_channel9_Configuration.Delay Timer 1 ms
V_channel9_Configuration.Delay Timer 2 ms
V_channel9_Configuration.Mirroring Enable
V_channel9_Configuration.Mirroring Channel Selection
V_channel9_Configuration.Mirroring Inversion
Channel10 Configuration
V_channel10_Configuration.IO Selection
V_channel10_Configuration.Delay Mode
V_channel10_Configuration.Delay Timer 1 ms
V_channel10_Configuration.Delay Timer 2 ms
V_channel10_Configuration.Mirroring Enable
V_channel10_Configuration.Mirroring Channel Selection
V_channel10_Configuration.Mirroring Inversion
Channel11 Configuration
V_channel11_Configuration.IO Selection
V_channel11_Configuration.Delay Mode
V_channel11_Configuration.Delay Timer 1 ms
V_channel11_Configuration.Delay Timer 2 ms
V_channel11_Configuration.Mirroring Enable
V_channel11_Configuration.Mirroring Channel Selection
V_channel11_Configuration.Mirroring Inversion
Channel12 Configuration
V_channel12_Configuration.IO Selection
V_channel12_Configuration.Delay Mode
V_channel12_Configuration.Delay Timer 1 ms
V_channel12_Configuration.Delay Timer 2 ms
V_channel12_Configuration.Mirroring Enable
V_channel12_Configuration.Mirroring Channel Selection
V_channel12_Configuration.Mirroring Inversion
Channel13 Configuration
V_channel13_Configuration.IO Selection
V_channel13_Configuration.Delay Mode
V_channel13_Configuration.Delay Timer 1 ms
V_channel13_Configuration.Delay Timer 2 ms
V_channel13_Configuration.Mirroring Enable
V_channel13_Configuration.Mirroring Channel Selection
V_channel13_Configuration.Mirroring Inversion
Channel14 Configuration
V_channel14_Configuration.IO Selection
V_channel14_Configuration.Delay Mode
V_channel14_Configuration.Delay Timer 1 ms
V_channel14_Configuration.Delay Timer 2 ms
V_channel14_Configuration.Mirroring Enable
V_channel14_Configuration.Mirroring Channel Selection
V_channel14_Configuration.Mirroring Inversion
Channel15 Configuration
V_channel15_Configuration.IO Selection
V_channel15_Configuration.Delay Mode
V_channel15_Configuration.Delay Timer 1 ms
V_channel15_Configuration.Delay Timer 2 ms
V_channel15_Configuration.Mirroring Enable
V_channel15_Configuration.Mirroring Channel Selection
V_channel15_Configuration.Mirroring Inversion
Channel16 Configuration
V_channel16_Configuration.IO Selection
V_channel16_Configuration.Delay Mode
V_channel16_Configuration.Delay Timer 1 ms
V_channel16_Configuration.Delay Timer 2 ms
V_channel16_Configuration.Mirroring Enable
V_channel16_Configuration.Mirroring Channel Selection
V_channel16_Configuration.Mirroring Inversion

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
IO Metrics Channels 1 to 8
V_IO_Metrics_Channel_1_to_8.Channel1 Count
V_IO_Metrics_Channel_1_to_8.Channel1 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel1 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel1 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel2 Count
V_IO_Metrics_Channel_1_to_8.Channel2 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel2 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel2 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel3 Count
V_IO_Metrics_Channel_1_to_8.Channel3 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel3 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel3 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel4 Count
V_IO_Metrics_Channel_1_to_8.Channel4 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel4 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel4 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel5 Count
V_IO_Metrics_Channel_1_to_8.Channel5 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel5 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel5 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel6 Count
V_IO_Metrics_Channel_1_to_8.Channel6 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel6 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel6 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel7 Count
V_IO_Metrics_Channel_1_to_8.Channel7 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel7 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel7 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel8 Count
V_IO_Metrics_Channel_1_to_8.Channel8 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel8 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel8 Totalizer Counter
IO Metrics Channels 9 to 16
V_IO_Metrics_Channel_9_to_16.Channel9 Count
V_IO_Metrics_Channel_9_to_16.Channel9 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel9 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel9 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel10 Count
V_IO_Metrics_Channel_9_to_16.Channel10 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel10 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel10 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel11 Count
V_IO_Metrics_Channel_9_to_16.Channel11 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel11 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel11 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel12 Count
V_IO_Metrics_Channel_9_to_16.Channel12 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel12 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel12 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel13 Count
V_IO_Metrics_Channel_9_to_16.Channel13 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel13 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel13 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel14 Count
V_IO_Metrics_Channel_9_to_16.Channel14 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel14 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel14 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel15 Count
V_IO_Metrics_Channel_9_to_16.Channel15 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel15 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel15 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel16 Count
V_IO_Metrics_Channel_9_to_16.Channel16 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel16 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel16 Totalizer Counter

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

## Commissioning Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameters Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
Selectable Metric Reset
V_Selectable_Metric_Reset.Channel1
V_Selectable_Metric_Reset.Channel2
V_Selectable_Metric_Reset.Channel3
V_Selectable_Metric_Reset.Channel4
V_Selectable_Metric_Reset.Channel5
V_Selectable_Metric_Reset.Channel6
V_Selectable_Metric_Reset.Channel7
V_Selectable_Metric_Reset.Channel8
V_Selectable_Metric_Reset.Channel9
V_Selectable_Metric_Reset.Channel10
V_Selectable_Metric_Reset.Channel11
V_Selectable_Metric_Reset.Channel12
V_Selectable_Metric_Reset.Channel13
V_Selectable_Metric_Reset.Channel14
V_Selectable_Metric_Reset.Channel15
V_Selectable_Metric_Reset.Channel16
V_Selectable_Metric_Reset.Channel1 Reset Count
V_Selectable_Metric_Reset.Channel2 Reset Count
V_Selectable_Metric_Reset.Channel3 Reset Count
V_Selectable_Metric_Reset.Channel4 Reset Count
V_Selectable_Metric_Reset.Channel5 Reset Count
V_Selectable_Metric_Reset.Channel6 Reset Count
V_Selectable_Metric_Reset.Channel7 Reset Count
V_Selectable_Metric_Reset.Channel8 Reset Count
V_Selectable_Metric_Reset.Channel9 Reset Count
V_Selectable_Metric_Reset.Channel10 Reset Count
V_Selectable_Metric_Reset.Channel11 Reset Count
V_Selectable_Metric_Reset.Channel12 Reset Count
V_Selectable_Metric_Reset.Channel13 Reset Count
V_Selectable_Metric_Reset.Channel14 Reset Count
V_Selectable_Metric_Reset.Channel15 Reset Count
V_Selectable_Metric_Reset.Channel16 Reset Count
Access Locks
V_DeviceAccessLocks.Local Parameterization
V_DeviceAccessLocks.Local User Interface
Vendor Specific Configuration
Channel1 Configuration
V_channel1_Configuration.IO Selection
V_channel1_Configuration.Delay Mode
V_channel1_Configuration.Delay Timer 1 ms
V_channel1_Configuration.Delay Timer 2 ms
V_channel1_Configuration.Mirroring Enable
V_channel1_Configuration.Mirroring Channel Selection
V_channel1_Configuration.Mirroring Inversion
Channel2 Configuration
V_channel2_Configuration.IO Selection
V_channel2_Configuration.Delay Mode
V_channel2_Configuration.Delay Timer 1 ms
V_channel2_Configuration.Delay Timer 2 ms
V_channel2_Configuration.Mirroring Enable
V_channel2_Configuration.Mirroring Channel Selection
V_channel2_Configuration.Mirroring Inversion
Channel3 Configuration
V_channel3_Configuration.IO Selection
V_channel3_Configuration.Delay Mode
V_channel3_Configuration.Delay Timer 1 ms
V_channel3_Configuration.Delay Timer 2 ms
V_channel3_Configuration.Mirroring Enable
V_channel3_Configuration.Mirroring Channel Selection
V_channel3_Configuration.Mirroring Inversion
Channel4 Configuration
V_channel4_Configuration.IO Selection
V_channel4_Configuration.Delay Mode
V_channel4_Configuration.Delay Timer 1 ms
V_channel4_Configuration.Delay Timer 2 ms
V_channel4_Configuration.Mirroring Enable
V_channel4_Configuration.Mirroring Channel Selection
V_channel4_Configuration.Mirroring Inversion
Channel5 Configuration
V_channel5_Configuration.IO Selection
V_channel5_Configuration.Delay Mode
V_channel5_Configuration.Delay Timer 1 ms
V_channel5_Configuration.Delay Timer 2 ms
V_channel5_Configuration.Mirroring Enable
V_channel5_Configuration.Mirroring Channel Selection
V_channel5_Configuration.Mirroring Inversion
Channel6 Configuration
V_channel6_Configuration.IO Selection
V_channel6_Configuration.Delay Mode
V_channel6_Configuration.Delay Timer 1 ms
V_channel6_Configuration.Delay Timer 2 ms
V_channel6_Configuration.Mirroring Enable
V_channel6_Configuration.Mirroring Channel Selection
V_channel6_Configuration.Mirroring Inversion
Channel7 Configuration
V_channel7_Configuration.IO Selection
V_channel7_Configuration.Delay Mode
V_channel7_Configuration.Delay Timer 1 ms
V_channel7_Configuration.Delay Timer 2 ms
V_channel7_Configuration.Mirroring Enable
V_channel7_Configuration.Mirroring Channel Selection
V_channel7_Configuration.Mirroring Inversion
Channel8 Configuration
V_channel8_Configuration.IO Selection
V_channel8_Configuration.Delay Mode
V_channel8_Configuration.Delay Timer 1 ms
V_channel8_Configuration.Delay Timer 2 ms
V_channel8_Configuration.Mirroring Enable
V_channel8_Configuration.Mirroring Channel Selection
V_channel8_Configuration.Mirroring Inversion
Channel9 Configuration
V_channel9_Configuration.IO Selection
V_channel9_Configuration.Delay Mode
V_channel9_Configuration.Delay Timer 1 ms
V_channel9_Configuration.Delay Timer 2 ms
V_channel9_Configuration.Mirroring Enable
V_channel9_Configuration.Mirroring Channel Selection
V_channel9_Configuration.Mirroring Inversion
Channel10 Configuration
V_channel10_Configuration.IO Selection
V_channel10_Configuration.Delay Mode
V_channel10_Configuration.Delay Timer 1 ms
V_channel10_Configuration.Delay Timer 2 ms
V_channel10_Configuration.Mirroring Enable
V_channel10_Configuration.Mirroring Channel Selection
V_channel10_Configuration.Mirroring Inversion
Channel11 Configuration
V_channel11_Configuration.IO Selection
V_channel11_Configuration.Delay Mode
V_channel11_Configuration.Delay Timer 1 ms
V_channel11_Configuration.Delay Timer 2 ms
V_channel11_Configuration.Mirroring Enable
V_channel11_Configuration.Mirroring Channel Selection
V_channel11_Configuration.Mirroring Inversion
Channel12 Configuration
V_channel12_Configuration.IO Selection
V_channel12_Configuration.Delay Mode
V_channel12_Configuration.Delay Timer 1 ms
V_channel12_Configuration.Delay Timer 2 ms
V_channel12_Configuration.Mirroring Enable
V_channel12_Configuration.Mirroring Channel Selection
V_channel12_Configuration.Mirroring Inversion
Channel13 Configuration
V_channel13_Configuration.IO Selection
V_channel13_Configuration.Delay Mode
V_channel13_Configuration.Delay Timer 1 ms
V_channel13_Configuration.Delay Timer 2 ms
V_channel13_Configuration.Mirroring Enable
V_channel13_Configuration.Mirroring Channel Selection
V_channel13_Configuration.Mirroring Inversion
Channel14 Configuration
V_channel14_Configuration.IO Selection
V_channel14_Configuration.Delay Mode
V_channel14_Configuration.Delay Timer 1 ms
V_channel14_Configuration.Delay Timer 2 ms
V_channel14_Configuration.Mirroring Enable
V_channel14_Configuration.Mirroring Channel Selection
V_channel14_Configuration.Mirroring Inversion
Channel15 Configuration
V_channel15_Configuration.IO Selection
V_channel15_Configuration.Delay Mode
V_channel15_Configuration.Delay Timer 1 ms
V_channel15_Configuration.Delay Timer 2 ms
V_channel15_Configuration.Mirroring Enable
V_channel15_Configuration.Mirroring Channel Selection
V_channel15_Configuration.Mirroring Inversion
Channel16 Configuration
V_channel16_Configuration.IO Selection
V_channel16_Configuration.Delay Mode
V_channel16_Configuration.Delay Timer 1 ms
V_channel16_Configuration.Delay Timer 2 ms
V_channel16_Configuration.Mirroring Enable
V_channel16_Configuration.Mirroring Channel Selection
V_channel16_Configuration.Mirroring Inversion

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
IO Metrics Channels 1 to 8
V_IO_Metrics_Channel_1_to_8.Channel1 Count
V_IO_Metrics_Channel_1_to_8.Channel1 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel1 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel1 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel2 Count
V_IO_Metrics_Channel_1_to_8.Channel2 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel2 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel2 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel3 Count
V_IO_Metrics_Channel_1_to_8.Channel3 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel3 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel3 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel4 Count
V_IO_Metrics_Channel_1_to_8.Channel4 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel4 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel4 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel5 Count
V_IO_Metrics_Channel_1_to_8.Channel5 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel5 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel5 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel6 Count
V_IO_Metrics_Channel_1_to_8.Channel6 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel6 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel6 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel7 Count
V_IO_Metrics_Channel_1_to_8.Channel7 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel7 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel7 Totalizer Counter
V_IO_Metrics_Channel_1_to_8.Channel8 Count
V_IO_Metrics_Channel_1_to_8.Channel8 Duration µs
V_IO_Metrics_Channel_1_to_8.Channel8 Events Per Minute
V_IO_Metrics_Channel_1_to_8.Channel8 Totalizer Counter
IO Metrics Channels 9 to 16
V_IO_Metrics_Channel_9_to_16.Channel9 Count
V_IO_Metrics_Channel_9_to_16.Channel9 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel9 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel9 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel10 Count
V_IO_Metrics_Channel_9_to_16.Channel10 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel10 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel10 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel11 Count
V_IO_Metrics_Channel_9_to_16.Channel11 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel11 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel11 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel12 Count
V_IO_Metrics_Channel_9_to_16.Channel12 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel12 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel12 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel13 Count
V_IO_Metrics_Channel_9_to_16.Channel13 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel13 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel13 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel14 Count
V_IO_Metrics_Channel_9_to_16.Channel14 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel14 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel14 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel15 Count
V_IO_Metrics_Channel_9_to_16.Channel15 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel15 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel15 Totalizer Counter
V_IO_Metrics_Channel_9_to_16.Channel16 Count
V_IO_Metrics_Channel_9_to_16.Channel16 Duration µs
V_IO_Metrics_Channel_9_to_16.Channel16 Events Per Minute
V_IO_Metrics_Channel_9_to_16.Channel16 Totalizer Counter

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.4.