**Release Notes**

This document contains information on current and past releases of the Safety Controller PC Interface software.

# Version 4.7.0 January 2022

**SC26 and XS26 Series Safety Controllers**

Added XS26-ISDd Model with Banner’s In-Series Diagnostics (ISD) Functionality.

* ISD Device Capability: RFID Safety Switches, *ISD Connect*, and E-Stop.
* *AutoDetect ISD* Configuration.

Added *ClickSet IP* to Models with Ethernet and Display*.*

Added .L5X File Support for Creating EtherNet/IP Connections with Labeled Tags.

## SC10 Safety Controller

# Added .L5X File Support for Creating EtherNet/IP Connections with Labeled Tags.

|  |  |
| --- | --- |
| **PC Interface** | **Safety Controller Supporting FID\*** |
| **Release Version** | **SC26 and XS26** | **SC10**  |
| 4.7.0 | FID 5 | FID 2 |
| 4.6.0 | FID 4 | FID 2 |
| 4.4.0 | FID 4 | FID 2 |
| 4.3.0 | FID 3 | FID 2 |
| 4.2.0 | FID 3 | FID 1 |
| 4.1.0 | FID 2 | FID 1 |
| 4.0.0 | FID 2 | FID 1 |
| 3.3.0 | FID 2 | N/A |
| 2.5.6 | FID 1 | N/A |

\* PC Interface is backward compatible with earlier FIDs.

# Version 4.6.0 November 2020

## SC10 Safety Controller

Added ISD Device Capability: ISD Connect.

Added ISD Sample Projects.

**SC26 and XS26 Series Safety Controllers**

Updated Sample Projects.

# Version 4.4.0 August 2020

## SC10 Safety Controller

Added ISD Device Capability: E-Stop.

**SC26 and XS26 Series Safety Controllers**

Added Press Control Functions.

Added Reset OR Logic Block.

Added One Shot Function Block.

Added Flash Rate Options for Status Outputs.

# Version 4.3.0 March 2020

## SC10 Safety Controller

Added Banner’s In-Series Diagnostics (ISD) Functionality.

Added ISD Device Capability: Door Switch (SI-RF Models).

Added PLC Tags/Labels File Creation.

Updated Two-Hand Control Connection Rules.

**SC26 and XS26 Series Safety Controllers**

Added PLC Tags/Labels File Creation.

# Version 4.2.0 Nov 2019

## SC10 Safety Controller

Added sample projects.

**SC26 and XS26 Series Safety Controllers**

Added SC-XM3 Fast Programming and Swapout feature.

# Version 4.1.0 May 2019

## SC10 Safety Controller

Added the following language options German, Spanish, French, Italian, Japanese, Korean, Portuguese, Chinese (Mainland), Chinese (Taiwan).

**SC26 and XS26 Series Safety Controllers**

No new features have been added since Version 3.3.0

# Version 4.0.0 April 2019

## SC10 Safety Controller

Initial launch of the SC10 product. Supports all features and functions as detailed in the Instruction Manual.

## SC26 and XS26 Series Safety Controllers

No new features have been added since Version 3.3.0

# Version 3.3.0 May 2018

**SC10 Safety Controller**

Not Applicable

## SC26 and XS26 Series Safety Controllers

New Features

 Added ability to toggle an input reference node in Simulation Mode.

 Added status output states in Functional View in Simulation Mode.

 Added milliseconds option to Muting Time Limit feature.

# Version 3.2.0 and earlier

**For details on these versions, choose the Help button Interface software. Then select the Release Notes option.**

 **on the toolbar of the PC**

