Version: V3.0 | Release Date: 2023-07-14

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Menus]

S15C
Vendor ID | 451 (0x01c3) |
Vendor Name | Banner Engineering Corporation
Vendor Text | More Sensors. More Solutions.
Vendor URL | www.bannerengineering.com/io-link
Device ID | 659467 (0x0a100b)
DeviceFamily | S15C Series
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x4000 (Common Application Profile: ?Unknown?), 0x8000 (Function Class: Device Identification), 0x8003 (Function Class: Device Diagnosis)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: yes
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 8.8 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_0 with 1 octet on-request data OPERATE = TYPE_2_V with 1 octet on-request data ISDU supported
Device Variant | S15C-B21-KQ
--- | ---
Description | Bimodal to IO-Link converter
Product ID | S15C-B21-KQ
Device Icon |
Device Symbol |
Connection Type | M12-4 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q

[Top]

## ProcessData id=PD_ProcessData

## ProcessDataIn "Process Data Input" id=PD_ProcessDataIn

bit length: 144
data type: 144-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Discrete1 Input State | true (1) = Discrete1 Input Active
2 | 1 | Boolean | false = Inactive, true = Active |  |  |  |  | Discrete2 Input State | true (1) = Discrete2 Input Active. Note - even if Discrete2 is configured as an output, the active state will be reflected at the input
3 | 16 | 32-bit Integer |  |  |  |  |  | Process Data Measurement 1 | Process Data Measurement 1 Value
4 | 48 | 32-bit Integer |  |  |  |  |  | Process Data Measurement 2 | Process Data Measurement 2 Value
5 | 80 | 32-bit Integer |  |  |  |  |  | Process Data Measurement 3 | Process Data Measurement 3 Value
6 | 112 | 32-bit Integer |  |  |  |  |  | Process Data Measurement 4 | Process Data Measurement 4 Value

Octet 0

bit offset | 143 | 142 | 141 | 140 | 139 | 138 | 137 | 136
subindex | 6
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 1

bit offset | 135 | 134 | 133 | 132 | 131 | 130 | 129 | 128
subindex | 6
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 2

bit offset | 127 | 126 | 125 | 124 | 123 | 122 | 121 | 120
subindex | 6
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 3

bit offset | 119 | 118 | 117 | 116 | 115 | 114 | 113 | 112
subindex | 6
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 111 | 110 | 109 | 108 | 107 | 106 | 105 | 104
subindex | 5
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 5

bit offset | 103 | 102 | 101 | 100 | 99 | 98 | 97 | 96
subindex | 5
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 6

bit offset | 95 | 94 | 93 | 92 | 91 | 90 | 89 | 88
subindex | 5
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 7

bit offset | 87 | 86 | 85 | 84 | 83 | 82 | 81 | 80
subindex | 5
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 8

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | 4
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 9

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | 4
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 10

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 4
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 11

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 4
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 12

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | 3
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 13

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 3
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 14

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 3
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 15

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 3
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 16

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 17

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 2 | 1

## ProcessDataOut "Process Data Output" id=PD_ProcessDataOut

bit length: 8
data type: 8-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Off, true = On |  |  |  |  | Discrete2 Output State | true (1) = Discrete2 Output Active

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 130 = Restore Factory Settings, 162 = Discovery Start, 163 = Discovery Stop, 164 = Reset All Metrics |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 130 = Restore Factory Settings, 162 = Discovery Start, 163 = Discovery Stop, 164 = Reset All Metrics
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  |  |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure, 5..255 = Reserved
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

data type: Array[6] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 6 | 6 |

## Standard Variable "Process Data Input" index=40 id=V_ProcessDataInput

data type: see ProcessDataIn!
access rights: ro
dynamic

## Standard Variable "Process Data Output" index=41 id=V_ProcessDataOutput

data type: see ProcessDataOut!
access rights: ro
dynamic
[Top]

## Variable "All-time Run Time" index=69 id=V_AllTimeRunTime

description: A read only run time counter (in hours) that tracks the total time the sensor has been running since manufacture
data type: 32-bit Record (subindex access not supported)
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time" index=70 id=V_ResetableRunTime

description: A read / write run time counter (in hours) that can be monitored or set by the user
data type: 32-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 |  |  |  |  | Run counter | Run counter

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Vendor Specific Configuration" index=76 id=V_Vendor_Specific_Configuration

description: Vendor Specific Configuration
data type: 96-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = Count, 2 = Duration, 3 = Events Per Minute, 4 = Counts Per Minute | 1 |  |  |  | PDin Measurement 1 Metric Selection | The Measurement Metric for PDin Measurement 1
2 | 8 | 8-bit UInteger | 0 = Port 1 | 0 |  |  |  | PDin Measurement 1 Port Selection | The Port Selected for PDin Measurement 1
3 | 16 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | PDin Measurement 1 Channel Selection | The Channel Selected for PDin Measurement 1
4 | 24 | 8-bit UInteger | 0 = Disabled, 1 = Count, 2 = Duration, 3 = Events Per Minute, 4 = Counts Per Minute | 3 |  |  |  | PDin Measurement 2 Metric Selection | The Measurement Metric for PDin Measurement 2
5 | 32 | 8-bit UInteger | 0 = Port 1 | 0 |  |  |  | PDin Measurement 2 Port Selection | The Port Selected for PDin Measurement 2
6 | 40 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | PDin Measurement 2 Channel Selection | The Channel Selected for PDin Measurement 2
7 | 48 | 8-bit UInteger | 0 = Disabled, 1 = Count, 2 = Duration, 3 = Events Per Minute, 4 = Counts Per Minute | 1 |  |  |  | PDin Measurement 3 Metric Selection | The Measurement Metric for PDin Measurement 3
8 | 56 | 8-bit UInteger | 0 = Port 1 | 0 |  |  |  | PDin Measurement 3 Port Selection | The Port Selected for PDin Measurement 3
9 | 64 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 1 |  |  |  | PDin Measurement 3 Channel Selection | The Channel Selected for PDin Measurement 3
10 | 72 | 8-bit UInteger | 0 = Disabled, 1 = Count, 2 = Duration, 3 = Events Per Minute, 4 = Counts Per Minute | 3 |  |  |  | PDin Measurement 4 Metric Selection | The Measurement Metric for PDin Measurement 4
11 | 80 | 8-bit UInteger | 0 = Port 1 | 0 |  |  |  | PDin Measurement 4 Port Selection | The Port Selected for PDin Measurement 4
12 | 88 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 1 |  |  |  | PDin Measurement 4 Channel Selection | The Channel Selected for PDin Measurement 4

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32
subindex | 12 | 11 | 10 | 9 | 8 | 7 | 6 | 5
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 4 | 3 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "All-time Run Time Event Time" index=78 id=V_AllTimeRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Event indicating the corresponding configured running time has elapsed.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Resetable Run Time Event Time" index=79 id=V_ResetableRunTimeEventTime

description: Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Event Time | Running time when an event will be raised indicating that service is required. Set to 0 to disable raising event.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "IO Metrics" index=80 id=V_IO_Metrics

description: IO Metrics Values
data type: 320-bit Record
access rights: ro
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete1 Count | Port 1 Discrete1 Count Value
2 | 32 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete1 Duration | Port 1 Discrete1 Duration Value
3 | 64 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete1 Events Per Minute | Port 1 Discrete1 Events Per Minute Value
4 | 96 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete1 Counts Per Minute | Port 1 Discrete1 Counts Per Minute Value
5 | 128 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete1 Totalizer Counter | Port 1 Discrete1 Totalizer Counter Value
6 | 160 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete2 Count | Port 1 Discrete2 Count Value
7 | 192 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete2 Duration | Port 1 Discrete2 Duration Value
8 | 224 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete2 Events Per Minute | Port 1 Discrete2 Events Per Minute Value
9 | 256 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete2 Counts Per Minute | Port 1 Discrete2 Counts Per Minute Value
10 | 288 | 32-bit Integer |  |  |  |  |  | Port 1 Discrete2 Totalizer Counter | Port 1 Discrete2 Totalizer Counter Value

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256
subindex | 10 | 10 | 10 | 10 | 9 | 9 | 9 | 9
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192
subindex | 8 | 8 | 8 | 8 | 7 | 7 | 7 | 7
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128
subindex | 6 | 6 | 6 | 6 | 5 | 5 | 5 | 5
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 4 | 4 | 4 | 4 | 3 | 3 | 3 | 3
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 1
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Selectable Metric Reset" index=81 id=V_Selectable_Metric_Reset

description: User can select which channel / Channels to reset
data type: 80-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port 1 Discrete1 | If set to [Reset], Port 1 Discrete1 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port1 Discrete1 Reset Count]
2 | 1 | Boolean | false = Do Not Reset, true = Reset | false |  |  |  | Port 1 Discrete2 | If set to [Reset], Port 1 Discrete2 metrics will be reset. Note - the Count value can be set to a non-zero value using [Port1 Discrete2 Reset Count]
3 | 16 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port 1 Discrete1 Reset Count |
4 | 48 | 32-bit Integer | 0..2147483647 | 0 |  |  |  | Port 1 Discrete2 Reset Count |

Octet 0

bit offset | 79 | 78 | 77 | 76 | 75 | 74 | 73 | 72
subindex | 4
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 1

bit offset | 71 | 70 | 69 | 68 | 67 | 66 | 65 | 64
subindex | 4
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 2

bit offset | 63 | 62 | 61 | 60 | 59 | 58 | 57 | 56
subindex | 4
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 3

bit offset | 55 | 54 | 53 | 52 | 51 | 50 | 49 | 48
subindex | 4
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 4

bit offset | 47 | 46 | 45 | 44 | 43 | 42 | 41 | 40
subindex | 3
element bit | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24

Octet 5

bit offset | 39 | 38 | 37 | 36 | 35 | 34 | 33 | 32
subindex | 3
element bit | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16

Octet 6

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 3
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 7

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 3
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 8

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 9

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 2 | 1

## Variable "Port1 Configuration" index=87 id=V_Port1_Configuration

description: Port1 Configuration
data type: 200-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = NPN Input, 1 = PNP Input | 1 |  |  |  | Discrete1 IO Selection |
2 | 8 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete1 Delay Mode | Discrete1 Delay Mode Selection
3 | 16 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 1 | Discrete1 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
4 | 48 | 32-bit Integer |  | 0 |  |  |  | Discrete1 Delay Timer 2 | Discrete1 Off Delay or Totalizer time.
5 | 80 | 8-bit UInteger | 0 = NPN Input, 1 = PNP Input, 2 = NPN Output with Pull Up, 3 = PNP Output with Pull Down, 4 = NPN Output Push Pull, 5 = PNP Output Push Pull | 1 |  |  |  | Discrete2 IO Selection |
6 | 88 | 8-bit UInteger | 0 = Disabled, 1 = On Off Delay, 2 = On One-shot, 3 = Off One-shot, 4 = On Pulse-stretcher, 5 = Off Pulse-stretcher, 6 = Totalizer, 7 = Retriggerable On One-shot, 8 = Retriggerable Off One-shot | 0 |  |  |  | Discrete2 Delay Mode | Discrete2 Delay Mode Selection
7 | 96 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 1 | Discrete2 On Delay, One-shot, Pulse-stretcher time or Totalizer Count
8 | 128 | 32-bit Integer |  | 0 |  |  |  | Discrete2 Delay Timer 2 | Discrete2 Off Delay or Totalizer time
9 | 160 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
10 | 168 | 8-bit UInteger | 0 = Port 1 | 0 |  |  |  | Mirroring Port Selection |
11 | 176 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Mirroring Channel Selection |
12 | 184 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |
13 | 192 | 8-bit UInteger | 0 = Slow, 1 = Medium, 2 = Fast | 1 |  |  |  | Counts Per Minute Mode | Counter Per Minute Mode Selection

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 199 - 192 | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136
subindex | 13 | 12 | 11 | 10 | 9 | 8 | 8 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72
subindex | 8 | 7 | 7 | 7 | 7 | 6 | 5 | 4
element bit | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8
subindex | 4 | 4 | 4 | 3 | 3 | 3 | 3 | 2
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0

octet | 24 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Discrete White Host Out Mirroring Configuration" index=91 id=V_Discrete_White_Host_Out_Mirroring_Configuration

description: Configuration parameters for mirroring Discrete1 or Discrete2 to White Host Out
data type: 48-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
2 | 8 | 8-bit UInteger | 0 = Port 1 | 0 |  |  |  | Mirroring Port Selection |
3 | 16 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Mirroring Channel Selection |
4 | 24 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |
5 | 32 | 8-bit UInteger | 0 = NPN Output, 1 = PNP Output | 1 |  |  |  | Mirroring Polarity |
6 | 40 | 8-bit UInteger | 0 = Output with Internal Pull Up / Down, 1 = Output Open Collector, 2 = Output Push Pull | 0 |  |  |  | Mirroring Output Type |

octet | 0 | 1 | 2 | 3 | 4 | 5 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 6 | 5 | 4 | 3 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 |

## Variable "Discrete Black Host Out Mirroring Configuration" index=92 id=V_Discrete_Black_Host_Out_Mirroring_Configuration

description: Configuration parameters for mirroring Discrete1 or Discrete2 to Black Host Out
data type: 48-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = Enabled | 0 |  |  |  | Mirroring Enable |
2 | 8 | 8-bit UInteger | 0 = Port 1 | 0 |  |  |  | Mirroring Port Selection |
3 | 16 | 8-bit UInteger | 0 = Discrete1, 1 = Discrete2 | 0 |  |  |  | Mirroring Channel Selection |
4 | 24 | 8-bit UInteger | 0 = Not Inverted, 1 = Inverted | 0 |  |  |  | Mirroring Inversion |
5 | 32 | 8-bit UInteger | 0 = NPN Output, 1 = PNP Output | 1 |  |  |  | Mirroring Polarity |
6 | 40 | 8-bit UInteger | 1 = Output Open Collector, 2 = Output Push Pull | 1 |  |  |  | Mirroring Output Type |

octet | 0 | 1 | 2 | 3 | 4 | 5 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 6 | 5 | 4 | 3 | 2 | 1 |
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
25376 (0x6320) | Error | Parameter error | Check data sheet and values
36000 (0x8ca0) | Warning | All-time Run Time Event | Event indicating the corresponding configured running time has elapsed.
36001 (0x8ca1) | Warning | Resetable Run Time Event | Event indicating the corresponding configured running time has elapsed.

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_ApplicationSpecificTag

Parameter Menu
V_Vendor_Specific_Configuration.PDin Measurement 1 Metric Selection, ro

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
V_IO_Metrics

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameter Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
Selectable Metric Reset
V_Selectable_Metric_Reset.Port 1 Discrete1
V_Selectable_Metric_Reset.Port 1 Discrete2
V_Selectable_Metric_Reset.Port 1 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port 1 Discrete2 Reset Count
Access Locks
V_DeviceAccessLocks.Local Parameterization Lock
V_DeviceAccessLocks.Local User Interface Lock
Vendor Specific Configuration
Port1 Configuration
V_Port1_Configuration.Discrete1 IO Selection
V_Port1_Configuration.Discrete1 Delay Mode
V_Port1_Configuration.Discrete1 Delay Timer 1 ms
V_Port1_Configuration.Discrete1 Delay Timer 2 ms
V_Port1_Configuration.Discrete2 IO Selection
V_Port1_Configuration.Discrete2 Delay Mode
V_Port1_Configuration.Discrete2 Delay Timer 1 ms
V_Port1_Configuration.Discrete2 Delay Timer 2 ms
V_Port1_Configuration.Mirroring Enable
V_Port1_Configuration.Mirroring Port Selection
V_Port1_Configuration.Mirroring Channel Selection
V_Port1_Configuration.Mirroring Inversion
V_Port1_Configuration.Counts Per Minute Mode
Discrete White Host Out Mirroring Configuration
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Enable
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Port Selection
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Channel Selection
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Inversion
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Polarity
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Output Type
Discrete Black Host Out Mirroring Configuration
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Enable
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Port Selection
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Channel Selection
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Inversion
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Polarity
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Output Type
PDin Measurement 1 Selection
V_Vendor_Specific_Configuration.PDin Measurement 1 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 1 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 1 Channel Selection
PDin Measurement 2 Selection
V_Vendor_Specific_Configuration.PDin Measurement 2 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 2 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 2 Channel Selection
PDin Measurement 3 Selection
V_Vendor_Specific_Configuration.PDin Measurement 3 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 3 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 3 Channel Selection
PDin Measurement 4 Selection
V_Vendor_Specific_Configuration.PDin Measurement 4 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 4 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 4 Channel Selection

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
V_IO_Metrics

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_ApplicationSpecificTag

Parameter Menu
Executable Commands
V_SystemCommand, Button:=130
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163
V_SystemCommand, Button:=164
Selectable Metric Reset
V_Selectable_Metric_Reset.Port 1 Discrete1
V_Selectable_Metric_Reset.Port 1 Discrete2
V_Selectable_Metric_Reset.Port 1 Discrete1 Reset Count
V_Selectable_Metric_Reset.Port 1 Discrete2 Reset Count
Access Locks
V_DeviceAccessLocks.Local Parameterization Lock
V_DeviceAccessLocks.Local User Interface Lock
Vendor Specific Configuration
Port1 Configuration
V_Port1_Configuration.Discrete1 IO Selection
V_Port1_Configuration.Discrete1 Delay Mode
V_Port1_Configuration.Discrete1 Delay Timer 1 ms
V_Port1_Configuration.Discrete1 Delay Timer 2 ms
V_Port1_Configuration.Discrete2 IO Selection
V_Port1_Configuration.Discrete2 Delay Mode
V_Port1_Configuration.Discrete2 Delay Timer 1 ms
V_Port1_Configuration.Discrete2 Delay Timer 2 ms
V_Port1_Configuration.Mirroring Enable
V_Port1_Configuration.Mirroring Port Selection
V_Port1_Configuration.Mirroring Channel Selection
V_Port1_Configuration.Mirroring Inversion
V_Port1_Configuration.Counts Per Minute Mode
Discrete White Host Out Mirroring Configuration
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Enable
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Port Selection
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Channel Selection
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Inversion
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Polarity
V_Discrete_White_Host_Out_Mirroring_Configuration.Mirroring Output Type
Discrete Black Host Out Mirroring Configuration
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Enable
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Port Selection
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Channel Selection
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Inversion
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Polarity
V_Discrete_Black_Host_Out_Mirroring_Configuration.Mirroring Output Type
PDin Measurement 1 Selection
V_Vendor_Specific_Configuration.PDin Measurement 1 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 1 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 1 Channel Selection
PDin Measurement 2 Selection
V_Vendor_Specific_Configuration.PDin Measurement 2 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 2 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 2 Channel Selection
PDin Measurement 3 Selection
V_Vendor_Specific_Configuration.PDin Measurement 3 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 3 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 3 Channel Selection
PDin Measurement 4 Selection
V_Vendor_Specific_Configuration.PDin Measurement 4 Metric Selection
V_Vendor_Specific_Configuration.PDin Measurement 4 Port Selection
V_Vendor_Specific_Configuration.PDin Measurement 4 Channel Selection

Observation Menu
V_ProcessDataInput
V_ProcessDataOutput
V_IO_Metrics

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Run Counters
V_AllTimeRunTime.Run counter * 0.25 h
V_ResetableRunTime.Run counter * 0.25 h
Event Timers
V_AllTimeRunTimeEventTime.Event Time * 0.25 h
V_ResetableRunTimeEventTime.Event Time * 0.25 h

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.