Version: V2.0 | Release Date: 2023-12-22

[Process Data]
[Standard Variables]
[Variables]
[Events]
[Process Data Formatting]
[Menus]

K50Z
Vendor ID | 451 (0x01c3) |
Vendor Name | Banner Engineering Corporation
Vendor Text | More Sensors. More Solutions.
Vendor URL | www.bannerengineering.com/io-link
Device ID | 851969 (0x0d0001)
DeviceFamily | K50Z
Features
Block Parameter | yes
Data Storage | yes
Profile Characteristic | 0x0001 (Device Profile: Smart Sensor), 0x8000 (Function Class: Device Identification), 0x8001 (Function Class: Binary Data Channel), 0x8002 (Function Class: Process Data Variables), 0x8003 (Function Class: Device Diagnosis), 0x8004 (Function Class: Teach-In Commands), 0x800a (Function Class: ?Unknown?)
Supported Access Locks | Parameter: yes, Data Storage: yes, Local Parameterization: yes, Local User Interface: yes
Communication
IO-Link Revision | V1.1
Transmission Rate | 38400 bit/s (COM2)
Minimum Cycle Time | 2.6 ms
SIO Mode Supported | yes
M-Sequence Capability | PREOPERATE = TYPE_0 with 1 octet on-request data OPERATE = TYPE_2_V with 1 octet on-request data ISDU supported
Device Variant | K50Z-FA2000KD-Q8
--- | ---
Description | 3D Time of Flight Sensor
Product ID | K50Z-FA2000KD-Q8
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC; Remote Input/BannerBus
Device Variant | K50Z-FA1000KD-Q8
Description | 3D Time of Flight Sensor
Product ID | K50Z-FA1000KD-Q8
Device Icon |
Device Symbol |
Connection Type | M12-5 connector
- pin 1 | brown; L+
- pin 2 | white; Other
- pin 3 | (light) blue; L-
- pin 4 | black; C/Q
- pin 5 | grey (slate); NC; Remote Input/BannerBus

[Top]

## ProcessData id=PD_ProcessData (condition V_Configuration.5 == 0)

## ProcessDataIn "Process Data In" id=PD_ProcessDataIn

bit length: 32
data type: 32-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 1 Output State | Channel 1 Output State
2 | 1 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 2 Output State | Channel 2 Output State
3 | 2 | Boolean | false = No target or Marginal, true = Stable |  |  |  |  | Stability (Zone 1) | Stability state (Zone 1)
4 | 3 | Boolean | false = No target or Marginal, true = Stable |  |  |  |  | Stability (Zone 2) | Stability state (Zone 2)
5 | 4 | 12-bit UInteger |  |  |  |  |  | Measurement 1 Value |
6 | 16 | 16-bit Integer |  |  |  |  |  | Measurement 2 Value |

Octet 0

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 6
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 6
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 5
element bit | 11 | 10 | 9 | 8 | 7 | 6 | 5 | 4

Octet 3

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | 5 | 4 | 3 | 2 | 1
element bit | 3 | 2 | 1 | 0 |  |  |  |

## ProcessDataOut "Process Data Out" id=PD_ProcessDataOut

bit length: 8
data type: 8-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Active, true = Inactive |  |  |  |  | Emitter Disable |

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

## ProcessData id=PD_ProcessDataWithoutBinary (condition V_Configuration.5 == 1)

## ProcessDataIn "Process Data In" id=PD_ProcessDataInWithoutBinary

bit length: 32
data type: 32-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 16-bit UInteger |  |  |  |  |  | Measurement 1 Value |
2 | 16 | 16-bit Integer |  |  |  |  |  | Measurement 2 Value |

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 2 | 2 | 1 | 1 |
element bit | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 |

## ProcessDataOut "Process Data Out" id=PD_ProcessDataOutWithoutBinary

bit length: 8
data type: 8-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Active, true = Inactive |  |  |  |  | Emitter Disable |

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

## ProcessData id=PD_ProcessDataMeasurement (condition V_Configuration.5 == 2)

## ProcessDataIn "Process Data In" id=PD_ProcessDataInMeasurement

bit length: 32
data type: 32-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 16 | 16-bit Integer |  |  |  |  |  | Measurement Value | The measurement device value
2 | 8 | 8-bit Integer |  |  |  |  |  | Measurement Scale | The measurement device scale
3 | 2 | Boolean | false = No target or Marginal, true = Stable |  |  |  |  | Stability | Stability state
4 | 1 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 2 Output State | Channel 2 Output State
5 | 0 | Boolean | false = Inactive, true = Active |  |  |  |  | Channel 1 Output State | Channel 1 Output State

Octet 0

bit offset | 31 | 30 | 29 | 28 | 27 | 26 | 25 | 24
subindex | 1
element bit | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8

Octet 1

bit offset | 23 | 22 | 21 | 20 | 19 | 18 | 17 | 16
subindex | 1
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 2

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | 2
element bit | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Octet 3

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 3 | 4 | 5

## ProcessDataOut "Process Data Out" id=PD_ProcessDataOutMeasurement

bit length: 8
data type: 8-bit Record (subindex access not supported)

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean | false = Active, true = Inactive |  |  |  |  | Emitter Disable |

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 1

[Top]

## Standard Variable "Direct Parameters 1" index=0 id=V_DirectParameters_1

data type: 128-bit Record
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  | ro |  |  | Reserved |
2 | 112 | 8-bit UInteger |  |  | ro |  |  | Master Cycle Time |
3 | 104 | 8-bit UInteger |  |  | ro |  |  | Min Cycle Time |
4 | 96 | 8-bit UInteger |  |  | ro |  |  | M-Sequence Capability |
5 | 88 | 8-bit UInteger |  | 17 | ro |  |  | IO-Link Version ID |
6 | 80 | 8-bit UInteger |  |  | ro |  |  | Process Data Input Length |
7 | 72 | 8-bit UInteger |  |  | ro |  |  | Process Data Output Length |
8 | 64 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 1 |
9 | 56 | 8-bit UInteger |  |  | ro |  |  | Vendor ID 2 |
10 | 48 | 8-bit UInteger |  |  | ro |  |  | Device ID 1 |
11 | 40 | 8-bit UInteger |  |  | ro |  |  | Device ID 2 |
12 | 32 | 8-bit UInteger |  |  | ro |  |  | Device ID 3 |
13 | 24 | 8-bit UInteger |  |  | ro |  |  | Reserved |
14 | 16 | 8-bit UInteger |  |  | ro |  |  | Reserved |
15 | 8 | 8-bit UInteger |  |  | ro |  |  | Reserved |
16 | 0 | 8-bit UInteger | 65 = SP1 Single Value Teach, 67 = SP1 Two Value Teach TP1, 68 = SP1 Two Value Teach TP2, 79 = S1 Exit Teach, 130 = Restore Factory Settings, 162 = Start discovery, 163 = Stop discovery |  | wo | X |  | Standard Command |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Direct Parameters 2" index=1 id=V_DirectParameters_2

data type: 128-bit Record
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 120 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 1 |
2 | 112 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 2 |
3 | 104 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 3 |
4 | 96 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 4 |
5 | 88 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 5 |
6 | 80 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 6 |
7 | 72 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 7 |
8 | 64 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 8 |
9 | 56 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 9 |
10 | 48 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 10 |
11 | 40 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 11 |
12 | 32 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 12 |
13 | 24 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 13 |
14 | 16 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 14 |
15 | 8 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 15 |
16 | 0 | 8-bit UInteger |  |  |  |  |  | Device Specific Parameter 16 |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64
subindex | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0

## Standard Variable "Standard Command" index=2 id=V_SystemCommand

data type: 8-bit UInteger
allowed values: 65 = SP1 Single Value Teach, 67 = SP1 Two Value Teach TP1, 68 = SP1 Two Value Teach TP2, 79 = S1 Exit Teach, 130 = Restore Factory Settings, 162 = Start discovery, 163 = Stop discovery
access rights: wo
modifies other variables

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Device Access Locks" index=12 id=V_DeviceAccessLocks

data type: 16-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | Boolean |  |  |  |  |  | Parameter (write) Access Lock |
2 | 1 | Boolean |  |  |  |  |  | Data Storage Lock |
3 | 2 | Boolean |  |  |  |  |  | Local Parameterization Lock |
4 | 3 | Boolean |  |  |  |  |  | Local User Interface Lock |

Octet 0

bit offset | 15 | 14 | 13 | 12 | 11 | 10 | 9 | 8
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / / | / / / / / /

Octet 1

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | / / / / / / | / / / / / / | 4 | 3 | 2 | 1

## Standard Variable "Vendor Name" index=16 id=V_VendorName

data type: 64-octet String UTF-8
default value: "Banner Engineering Corporation"
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Vendor Text" index=17 id=V_VendorText

data type: 64-octet String UTF-8
default value: "More Sensors. More Solutions."
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Name" index=18 id=V_ProductName

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product ID" index=19 id=V_ProductID

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Product Text" index=20 id=V_ProductText

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Serial Number" index=21 id=V_SerialNumber

data type: 16-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Hardware Version" index=22 id=V_HardwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Firmware Version" index=23 id=V_FirmwareRevision

data type: 64-octet String UTF-8
access rights: ro

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 511 - 504 | 503 - 496 | 495 - 488 | 487 - 480 | 479 - 472 | 471 - 464 | 463 - 456 | 455 - 448

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 447 - 440 | 439 - 432 | 431 - 424 | 423 - 416 | 415 - 408 | 407 - 400 | 399 - 392 | 391 - 384

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 383 - 376 | 375 - 368 | 367 - 360 | 359 - 352 | 351 - 344 | 343 - 336 | 335 - 328 | 327 - 320

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 319 - 312 | 311 - 304 | 303 - 296 | 295 - 288 | 287 - 280 | 279 - 272 | 271 - 264 | 263 - 256

octet | 32 | 33 | 34 | 35 | 36 | 37 | 38 | 39
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 40 | 41 | 42 | 43 | 44 | 45 | 46 | 47
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 48 | 49 | 50 | 51 | 52 | 53 | 54 | 55
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 56 | 57 | 58 | 59 | 60 | 61 | 62 | 63
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Application Specific Tag" index=24 id=V_ApplicationSpecificTag

data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Standard Variable "Device Status" index=36 id=V_DeviceStatus

data type: 8-bit UInteger
allowed values: 0 = Device is OK, 1 = Maintenance required, 2 = Out of specification, 3 = Functional check, 4 = Failure, 5..255 = Reserved
access rights: ro
dynamic

octet | 0 |
bit offset | 7 - 0 |
element bit | 7 - 0 |

## Standard Variable "Detailed Device Status" index=37 id=V_DetailedDeviceStatus

data type: Array[6] of 3-octet OctetString (subindex access not supported)
access rights: ro
dynamic

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 143 - 136 | 135 - 128 | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80
subindex | 1 | 1 | 1 | 2 | 2 | 2 | 3 | 3

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16
subindex | 3 | 4 | 4 | 4 | 5 | 5 | 5 | 6

octet | 16 | 17 |
bit offset | 15 - 8 | 7 - 0 |
subindex | 6 | 6 |

## Standard Variable "Process Data Input" index=40 id=V_ProcessDataInput

data type: see ProcessDataIn!
access rights: ro
dynamic

## Standard Variable "Process Data Output" index=41 id=V_ProcessDataOutput

data type: see ProcessDataOut!
access rights: ro
dynamic
[Top]

## Variable "Function Tag" index=25 id=V_FunctionTag

data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Location Tag" index=26 id=V_LocationTag

data type: 32-octet String UTF-8
access rights: rw

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 255 - 248 | 247 - 240 | 239 - 232 | 231 - 224 | 223 - 216 | 215 - 208 | 207 - 200 | 199 - 192

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 191 - 184 | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 | 23
bit offset | 127 - 120 | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64

octet | 24 | 25 | 26 | 27 | 28 | 29 | 30 | 31
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Teach-in Channel" index=58 id=V_TeachChannel

description: The parameter 'Teach-in Channel' allows addressing the particular BDC or a set of BDCs for which the teach-in commands apply.
data type: 8-bit Record (subindex access not supported)
access rights: rw
excluded from data storage

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Default, 1 = BDC1, 2 = BDC2 | 0 |  |  |  | Teach-in Channel | Teach-in Channel

octet | 0 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "Teach-in Status" index=59 id=V_TeachStatus

description: The parameter 'Teach-in Status' provides feedback on the status and the results of the teach-in activities.
data type: 8-bit Record (subindex access not supported)
access rights: ro
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 4-bit UInteger | 0 = IDLE, 1 = SP1 SUCCESS, 4 = WAIT FOR COMMAND, 5 = BUSY, 7 = ERROR |  |  |  |  | Teach State | Teach State
2 | 4 | Boolean |  |  |  |  |  | SP1 TP1 | SP1 TP1
3 | 5 | Boolean |  |  |  |  |  | SP1 TP2 | SP1 TP2

Octet 0

bit offset | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
subindex | / / / / / / | / / / / / / | 3 | 2 | 1
element bit |  |  |  |  | 3 | 2 | 1 | 0

## Variable "BDC1 Setpoints" index=60 id=V_BDC1_Setpoints

description: The reference value used for sensor switching (See IOL Smart Sensor Profile 9.2.5)
data type: 64-bit Record (subindex access not supported)
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Setpoint SP1 | Switch point
2 | 0 | 32-bit Integer |  |  |  |  |  | Setpoint SP2 | In Two Point Window (FGS) teach, defines the second switching point. In other teach modes, SP2 is unused and must be written to 0.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "BDC1 Configuration" index=61 id=V_BDC1_Configuration

description: Parameter coding of the Setpoint and Switchpoint parameter. (See IOL Smart Sensor Profile 9.2.6)
data type: 32-bit Record
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 8-bit UInteger | 0 = Light Operate (LO), 1 = Dark Operate (DO) | 0 |  |  |  | Switchpoint Logic | Set LO/DO selection
2 | 16 | 8-bit UInteger | 1 = One-Point Object SET, 128 = One-Point static BGS, 129 = Two-Point Window (FGS) | 1 |  |  |  | BDC Mode | Defines how the binary switching information is created depending on Setpoint parameters (SP1, SP2) and the current measurement value
3 | 0 | 16-bit Integer |  | 0 |  |  |  | Hysteresis | The hysteresis value for the switchpoint. A value of 0 will result in automatically calculated hysteresis.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "BDC2 Setpoints" index=62 id=V_BDC2_Setpoints

description: The reference value used for sensor switching (See IOL Smart Sensor Profile 9.2.5)
data type: 64-bit Record (subindex access not supported)
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Setpoint SP1 | Switch point
2 | 0 | 32-bit Integer |  |  |  |  |  | Setpoint SP2 | In Two Point Window (FGS) teach, defines the second switching point. In other teach modes, SP2 is unused and must be written to 0.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "BDC2 Configuration" index=63 id=V_BDC2_Configuration

description: Parameter coding of the Setpoint and Switchpoint parameter. (See IOL Smart Sensor Profile 9.2.6)
data type: 32-bit Record
access rights: rw
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 24 | 8-bit UInteger | 0 = Light Operate (LO), 1 = Dark Operate (DO) | 0 |  |  |  | Switchpoint Logic | Set LO/DO selection
2 | 16 | 8-bit UInteger | 1 = One-Point Object SET, 128 = One-Point static BGS, 129 = Two-Point Window (FGS) | 1 |  |  |  | BDC Mode | Defines how the binary switching information is created depending on Setpoint parameters (SP1, SP2) and the current measurement value
3 | 0 | 16-bit Integer |  | 0 |  |  |  | Hysteresis | The hysteresis value for the switchpoint. A value of 0 will result in automatically calculated hysteresis.

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 2 | 3 | 3 |
element bit | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 |

## Variable "Configuration" index=64 id=V_Configuration

description: User selectable settings
data type: 72-bit Record
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Reduced Resolution, Fast, 1 = Reduced Resolution, Medium, 2 = Reduced Resolution, Slow, 3 = Fast, 4 = Medium, 5 = Slow | 3 |  |  |  | Response Speed | Response Speed of discrete output
2 | 8 | 8-bit UInteger | 0 = Remote Teach Input, 1 = Emitter On, 2 = Emitter Off, 3 = Disabled | 0 |  |  |  | Remote Input Mode | Remote Input Mode
3 | 16 | 8-bit UInteger | 0 = Independent Output, 1 = Complementary Output, 2 = Pulse Frequency Modulation | 0 |  |  |  | Secondary Output Function | The function of the secondary output channel
4 | 24 | 16-bit UInteger |  | 0 |  |  |  | IOL Filter Time | Time to average IOL process data measurement between updates.
5 | 40 | 8-bit UInteger | 0 = Include, 1 = Don't Include, 2 = Measurement Device | 0 |  |  |  | Include Binary Data in Process Data | Whether binary data (output and valid states) should be included with input process data.
6 | 48 | 8-bit UInteger | 0 = Disabled, 1 = Excess Gain (Zone 1), 2 = Excess Gain (Zone 2), 3 = Excess Gain / 10 (Zone 1), 4 = Excess Gain / 10 (Zone 2), 5 = Measurement Value (Zone 1), 6 = Measurement Value (Zone 2) | 5 |  |  |  | Measurement 1 Selection | Determines which value to place into process data measurement 1
7 | 56 | 8-bit UInteger | 0 = Disabled, 1 = Excess Gain (Zone 1), 2 = Excess Gain (Zone 2), 3 = Excess Gain / 10 (Zone 1), 4 = Excess Gain / 10 (Zone 2), 5 = Measurement Value (Zone 1), 6 = Measurement Value (Zone 2) | 6 |  |  |  | Measurement 2 Selection | Determines which value to place into process data measurement 2
8 | 64 | 8-bit UInteger | 0 = Zone 1, 1 = Zone 2 | 0 |  |  |  | Digital Measuring Sensor Zone Selection | Select Zone for Digitial Measuring Sensor mode

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8
subindex | 8 | 7 | 6 | 5 | 4 | 4 | 3 | 2
element bit | 7 - 0 | 7 - 0 | 7 - 0 | 7 - 0 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0

octet | 8 |
bit offset | 7 - 0 |
subindex | 1 |
element bit | 7 - 0 |

## Variable "BDC1 Vendor Specific Configuration" index=65 id=V_BDC1_Vendor_Specific_Configuration

description: Vendor specific user selectable BDC1 settings
data type: 112-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = On-Off Delay, 2 = Oneshot | 0 |  |  |  | Delay Mode | Delay Mode selection
2 | 8 | 32-bit UInteger | 0..90000 | 0 |  |  |  | Delay Time On/Oneshot | On delay, oneshot time.
3 | 40 | 32-bit UInteger | 0..90000 | 0 |  |  |  | Delay Time Off | Off delay time. In oneshot mode, this parameter must be written as 0.
4 | 72 | 8-bit UInteger | 0 = Auto, 1 = User Selected | 0 |  |  |  | Teach Offset Mode | Select whether to use automatic or fixed offset in Object SET or Window (FGS) mode. All other modes must be set to Auto
5 | 80 | 32-bit Integer |  | 0 |  |  |  | User Teach Offset | The user selected teach offset. In Object SET or Window (FGS) mode this value can be either positive or negative. In all other teach modes this value must be written as 0

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48
subindex | 5 | 5 | 5 | 5 | 4 | 3 | 3 | 3
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8

octet | 8 | 9 | 10 | 11 | 12 | 13 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 2 | 2 | 2 | 2 | 1 |
element bit | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "BDC2 Vendor Specific Configuration" index=66 id=V_BDC2_Vendor_Specific_Configuration

description: Vendor Specific user selectable BDC2 output settings
data type: 112-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 8-bit UInteger | 0 = Disabled, 1 = On-Off Delay, 2 = Oneshot | 0 |  |  |  | Delay Mode | Delay Mode selection
2 | 8 | 32-bit UInteger | 0..90000 | 0 |  |  |  | Delay Time On/Oneshot | On delay, oneshot time.
3 | 40 | 32-bit UInteger | 0..90000 | 0 |  |  |  | Delay Time Off | Off delay time. In oneshot mode, this parameter must be written as 0.
4 | 72 | 8-bit UInteger | 0 = Auto, 1 = User Selected | 0 |  |  |  | Teach Offset Mode | Select whether to use automatic or fixed offset in Object SET or Window (FGS) mode. All other modes must be set to Auto
5 | 80 | 32-bit Integer |  | 0 |  |  |  | User Teach Offset | The user selected teach offset. In Object SET or Window (FGS) mode this value can be either positive or negative. In all other teach modes this value must be written as 0

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48
subindex | 5 | 5 | 5 | 5 | 4 | 3 | 3 | 3
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8

octet | 8 | 9 | 10 | 11 | 12 | 13 |
bit offset | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 2 | 2 | 2 | 2 | 1 |
element bit | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 |

## Variable "Status" index=67 id=V_Status

description: Status
data type: 184-bit Record
access rights: ro
dynamic

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer |  |  |  |  |  | Measurement Value (Zone 1) |
2 | 32 | 32-bit Integer |  |  |  |  |  | Excess Gain (Zone 1) |
3 | 64 | 8-bit UInteger | 0 = No target exists, 1 = Marginal signal, 2 = Stable |  |  |  |  | Stability (Zone 1) | Stability state (Zone 1)
4 | 72 | 32-bit Integer |  |  |  |  |  | Measurement Value (Zone 2) |
5 | 104 | 32-bit Integer |  |  |  |  |  | Excess Gain (Zone 2) |
6 | 136 | 8-bit UInteger | 0 = No target exists, 1 = Marginal signal, 2 = Stable |  |  |  |  | Stability (Zone 2) | Stability state (Zone 2)
7 | 144 | 8-bit UInteger | 0 = Active, 1 = Inactive |  |  |  |  | Emitter Status | Emitter Status
8 | 152 | 16-bit Integer |  |  |  |  |  | Temperature | Internal temperature measurement for the device.
9 | 168 | 16-bit Integer |  |  |  |  |  | Last Taught Temperature | Internal temperature measurement the last time the device was taught.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 183 - 176 | 175 - 168 | 167 - 160 | 159 - 152 | 151 - 144 | 143 - 136 | 135 - 128 | 127 - 120
subindex | 9 | 9 | 8 | 8 | 7 | 6 | 5 | 5
element bit | 15 - 8 | 7 - 0 | 15 - 8 | 7 - 0 | 7 - 0 | 7 - 0 | 31 - 24 | 23 - 16

octet | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15
bit offset | 119 - 112 | 111 - 104 | 103 - 96 | 95 - 88 | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56
subindex | 5 | 5 | 4 | 4 | 4 | 4 | 3 | 2
element bit | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 7 - 0 | 31 - 24

octet | 16 | 17 | 18 | 19 | 20 | 21 | 22 |
bit offset | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 2 | 2 | 2 | 1 | 1 | 1 | 1 |
element bit | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "Pulse Frequency Configuration" index=71 id=V_PulseFrequencyConfiguration

description: BDC2 Only - Configuration of pulse frequency ranges.
data type: 64-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 1..100000 | 100 |  |  |  | Near Frequency | BDC2 Only - The frequency corresponding to a target at the near limit of the sensing range.
2 | 32 | 32-bit Integer | 1..100000 | 600 |  |  |  | Far Frequency | BDC2 Only - The frequency corresponding to a target at the far limit of the sensing range.

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 1
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Pulse Frequency Setpoints" index=78 id=V_PulseFrequencySetpoints

description: BDC2 Only - Distances used for scaling of Pulse Frequency output.
data type: 64-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 32 | 32-bit Integer |  |  |  |  |  | Setpoint SP1 | BDC2 Only - Switch point 1 for pulse frequency window
2 | 0 | 32-bit Integer |  |  |  |  |  | Setpoint SP2 | BDC2 Only - Switch point 2 for pulse frequency window

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

## Variable "Pulse Frequency LOS Frequency" index=79 id=V_PulseFrequencyLOSFrequency

description: BDC2 Only - Frequency used to indicate Loss-of-Signal
data type: 32-bit Record (subindex access not supported)
access rights: rw

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 0 | 32-bit Integer | 1..100000 | 50 |  |  |  | Pulse Frequency LOS Frequency | BDC2 Only - Frequency used to indicate Loss-of-Signal

octet | 0 | 1 | 2 | 3 |
bit offset | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 1 | 1 | 1 | 1 |
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 |

## Variable "MDC Descriptor" index=16512 id=V_MDCDescriptor

description: Measuring Data Channel Descriptor - refer to Smart Sensor Profile 2nd Ed.
data type: 88-bit Record
access rights: ro

subindex | bit offset | data type | allowed values | default value | acc. restr. | mod. other var. | excl. from DS | name | description
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 56 | 32-bit Integer |  |  |  |  |  | MDC Descr - Lower Limit |
2 | 24 | 32-bit Integer |  |  |  |  |  | MDC Descr - Upper Limit |
3 | 8 | 16-bit UInteger | 1010 = m |  |  |  |  | MDC Descr - Unit |
4 | 0 | 8-bit Integer |  |  |  |  |  | MDC Descr - Scale |

octet | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7
bit offset | 87 - 80 | 79 - 72 | 71 - 64 | 63 - 56 | 55 - 48 | 47 - 40 | 39 - 32 | 31 - 24
subindex | 1 | 1 | 1 | 1 | 2 | 2 | 2 | 2
element bit | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0 | 31 - 24 | 23 - 16 | 15 - 8 | 7 - 0

octet | 8 | 9 | 10 |
bit offset | 23 - 16 | 15 - 8 | 7 - 0 |
subindex | 3 | 3 | 4 |
element bit | 15 - 8 | 7 - 0 | 7 - 0 |

[Top]

## Events

Code | Type | Name | Description
--- | --- | --- | ---
25376 (0x6320) | Error | Parameter error | Check data sheet and values
36003 (0x8ca3) | Notification | Teach Completed Event | Event indicating a teach has been completed.
36004 (0x8ca4) | Notification | Factory Settings Restored Event | Event indicating that the factory settings have been restored.
36005 (0x8ca5) | Notification | Teach Coerced Event | Event indicating a taught condition resulted in a setpoint being coerced. Setpoints were updated.
36007 (0x8ca7) | Notification | Teach Failed Event | Event indicating an invalid target condition was attempted to be taught. Setpoints were not updated.
36097 (0x8d01) | Error | System Fault Event | Contact Banner Engineering to resolve.

[Top]

## Process Data Formatting

Formatting for Process Data id=PD_ProcessDataIn
Subindex 1:
Subindex 2:
Subindex 3:
Subindex 4:
Subindex 5:
Subindex 6:

Formatting for Process Data id=PD_ProcessDataOut
Subindex 1:

Formatting for Process Data id=PD_ProcessDataInWithoutBinary
Subindex 1:
Subindex 2:

Formatting for Process Data id=PD_ProcessDataOutWithoutBinary
Subindex 1:

Formatting for Process Data id=PD_ProcessDataInMeasurement
Subindex 1: * 0.001 m
Subindex 3:
Subindex 4:
Subindex 5:

Formatting for Process Data id=PD_ProcessDataOutMeasurement
Subindex 1:

[Top]

## Observer Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_ApplicationSpecificTag

Parameter Menu
V_Configuration.Include Binary Data in Process Data, ro
V_Configuration.Measurement 1 Selection, ro
V_Configuration.Measurement 2 Selection, ro

Observation Menu
If V_Configuration.5 = 0:
Process Data
V_ProcessDataInput.1
V_ProcessDataInput.2
V_ProcessDataInput.3
V_ProcessDataInput.4
V_ProcessDataInput.5
V_ProcessDataInput.6
V_ProcessDataOutput
If V_Configuration.5 = 1:
Process Data
V_ProcessDataInput.1 mm
V_ProcessDataInput.2 %
V_ProcessDataOutput
If V_Configuration.5 = 2:
Process Data
V_ProcessDataInput.1 * 0.001 m
V_ProcessDataInput.3
V_ProcessDataInput.4
V_ProcessDataInput.5
V_ProcessDataOutput

## Maintenance Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_HardwareRevision
V_ApplicationSpecificTag
V_FunctionTag
V_LocationTag

Parameter Menu
Device Access Locks
V_DeviceAccessLocks.Local Parameterization Lock
Teach-in Channel
V_TeachChannel
BDC1 Setpoints
V_BDC1_Setpoints.Setpoint SP1 mm
V_BDC1_Setpoints.Setpoint SP2 mm
BDC1 Configuration
V_BDC1_Configuration.Switchpoint Logic
V_BDC1_Configuration.BDC Mode
V_BDC1_Configuration.Hysteresis mm
BDC1 Vendor Specific Configuration
V_BDC1_Vendor_Specific_Configuration.Delay Mode
V_BDC1_Vendor_Specific_Configuration.Delay Time On/Oneshot ms
V_BDC1_Vendor_Specific_Configuration.Delay Time Off ms
V_BDC1_Vendor_Specific_Configuration.Teach Offset Mode
V_BDC1_Vendor_Specific_Configuration.User Teach Offset mm
BDC2 Setpoints
V_BDC2_Setpoints.Setpoint SP1 mm
V_BDC2_Setpoints.Setpoint SP2 mm
BDC2 Configuration
V_BDC2_Configuration.Switchpoint Logic
V_BDC2_Configuration.BDC Mode
V_BDC2_Configuration.Hysteresis mm
BDC2 Vendor Specific Configuration
V_BDC2_Vendor_Specific_Configuration.Delay Mode
V_BDC2_Vendor_Specific_Configuration.Delay Time On/Oneshot ms
V_BDC2_Vendor_Specific_Configuration.Delay Time Off ms
V_BDC2_Vendor_Specific_Configuration.Teach Offset Mode
V_BDC2_Vendor_Specific_Configuration.User Teach Offset mm
Configuration
V_Configuration.Response Speed
V_Configuration.Remote Input Mode
V_Configuration.Secondary Output Function
V_Configuration.IOL Filter Time ms
V_Configuration.Include Binary Data in Process Data
V_Configuration.Measurement 1 Selection
V_Configuration.Measurement 2 Selection
V_Configuration.Digital Measuring Sensor Zone Selection
Pulse Frequency Configuration
V_PulseFrequencySetpoints.Setpoint SP1 mm
V_PulseFrequencySetpoints.Setpoint SP2 mm
V_PulseFrequencyConfiguration.Near Frequency Hz
V_PulseFrequencyConfiguration.Far Frequency Hz
V_PulseFrequencyLOSFrequency.Pulse Frequency LOS Frequency Hz
System Commands
V_SystemCommand, Button:=65
V_SystemCommand, Button:=130
V_SystemCommand, Button:=67
V_SystemCommand, Button:=68
V_SystemCommand, Button:=79
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163

Observation Menu
If V_Configuration.5 = 0:
Process Data
V_ProcessDataInput.1
V_ProcessDataInput.2
V_ProcessDataInput.3
V_ProcessDataInput.4
V_ProcessDataInput.5
V_ProcessDataInput.6
V_ProcessDataOutput
If V_Configuration.5 = 1:
Process Data
V_ProcessDataInput.1 mm
V_ProcessDataInput.2 %
V_ProcessDataOutput
If V_Configuration.5 = 2:
Process Data
V_ProcessDataInput.1 * 0.001 m
V_ProcessDataInput.3
V_ProcessDataInput.4
V_ProcessDataInput.5
V_ProcessDataOutput

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Teach-in Status
V_TeachStatus.Teach State
V_TeachStatus.SP1 TP1
V_TeachStatus.SP1 TP2
Status
V_Status.Measurement Value (Zone 1) mm
V_Status.Excess Gain (Zone 1)
V_Status.Stability (Zone 1)
V_Status.Measurement Value (Zone 2) mm
V_Status.Excess Gain (Zone 2)
V_Status.Stability (Zone 2)
V_Status.Emitter Status
V_Status.Temperature * 0.1 °C
V_Status.Last Taught Temperature * 0.1 °C
Measuring Data Channel
V_MDCDescriptor.MDC Descr - Lower Limit * 0.001 m
V_MDCDescriptor.MDC Descr - Upper Limit * 0.001 m
V_MDCDescriptor.MDC Descr - Scale
V_MDCDescriptor.MDC Descr - Unit

## Specialist Menus

Identification Menu
V_VendorName
V_VendorText
V_ProductName
V_ProductID
V_ProductText
V_SerialNumber
V_FirmwareRevision
V_HardwareRevision
V_ApplicationSpecificTag
V_FunctionTag
V_LocationTag

Parameter Menu
Device Access Locks
V_DeviceAccessLocks.Local Parameterization Lock
Teach-in Channel
V_TeachChannel
BDC1 Setpoints
V_BDC1_Setpoints.Setpoint SP1 mm
V_BDC1_Setpoints.Setpoint SP2 mm
BDC1 Configuration
V_BDC1_Configuration.Switchpoint Logic
V_BDC1_Configuration.BDC Mode
V_BDC1_Configuration.Hysteresis mm
BDC1 Vendor Specific Configuration
V_BDC1_Vendor_Specific_Configuration.Delay Mode
V_BDC1_Vendor_Specific_Configuration.Delay Time On/Oneshot ms
V_BDC1_Vendor_Specific_Configuration.Delay Time Off ms
V_BDC1_Vendor_Specific_Configuration.Teach Offset Mode
V_BDC1_Vendor_Specific_Configuration.User Teach Offset mm
BDC2 Setpoints
V_BDC2_Setpoints.Setpoint SP1 mm
V_BDC2_Setpoints.Setpoint SP2 mm
BDC2 Configuration
V_BDC2_Configuration.Switchpoint Logic
V_BDC2_Configuration.BDC Mode
V_BDC2_Configuration.Hysteresis mm
BDC2 Vendor Specific Configuration
V_BDC2_Vendor_Specific_Configuration.Delay Mode
V_BDC2_Vendor_Specific_Configuration.Delay Time On/Oneshot ms
V_BDC2_Vendor_Specific_Configuration.Delay Time Off ms
V_BDC2_Vendor_Specific_Configuration.Teach Offset Mode
V_BDC2_Vendor_Specific_Configuration.User Teach Offset mm
Configuration
V_Configuration.Response Speed
V_Configuration.Remote Input Mode
V_Configuration.Secondary Output Function
V_Configuration.IOL Filter Time ms
V_Configuration.Include Binary Data in Process Data
V_Configuration.Measurement 1 Selection
V_Configuration.Measurement 2 Selection
V_Configuration.Digital Measuring Sensor Zone Selection
Pulse Frequency Configuration
V_PulseFrequencySetpoints.Setpoint SP1 mm
V_PulseFrequencySetpoints.Setpoint SP2 mm
V_PulseFrequencyConfiguration.Near Frequency Hz
V_PulseFrequencyConfiguration.Far Frequency Hz
V_PulseFrequencyLOSFrequency.Pulse Frequency LOS Frequency Hz
System Commands
V_SystemCommand, Button:=65
V_SystemCommand, Button:=130
V_SystemCommand, Button:=67
V_SystemCommand, Button:=68
V_SystemCommand, Button:=79
V_SystemCommand, Button:=162
V_SystemCommand, Button:=163

Observation Menu
If V_Configuration.5 = 0:
Process Data
V_ProcessDataInput.1
V_ProcessDataInput.2
V_ProcessDataInput.3
V_ProcessDataInput.4
V_ProcessDataInput.5
V_ProcessDataInput.6
V_ProcessDataOutput
If V_Configuration.5 = 1:
Process Data
V_ProcessDataInput.1 mm
V_ProcessDataInput.2 %
V_ProcessDataOutput
If V_Configuration.5 = 2:
Process Data
V_ProcessDataInput.1 * 0.001 m
V_ProcessDataInput.3
V_ProcessDataInput.4
V_ProcessDataInput.5
V_ProcessDataOutput

Diagnosis Menu
Device Status
V_DeviceStatus
V_DetailedDeviceStatus
Teach-in Status
V_TeachStatus.Teach State
V_TeachStatus.SP1 TP1
V_TeachStatus.SP1 TP2
Status
V_Status.Measurement Value (Zone 1) mm
V_Status.Excess Gain (Zone 1)
V_Status.Stability (Zone 1)
V_Status.Measurement Value (Zone 2) mm
V_Status.Excess Gain (Zone 2)
V_Status.Stability (Zone 2)
V_Status.Emitter Status
V_Status.Temperature * 0.1 °C
V_Status.Last Taught Temperature * 0.1 °C
Measuring Data Channel
V_MDCDescriptor.MDC Descr - Lower Limit * 0.001 m
V_MDCDescriptor.MDC Descr - Upper Limit * 0.001 m
V_MDCDescriptor.MDC Descr - Scale
V_MDCDescriptor.MDC Descr - Unit

Note: This page shows the content of an IODD file transformed into HTML format. In the case of disparity between this and the XML view, the content of the XML file takes precedence.
Created by IODD Viewer V1.1.