This folder contains the code that allows a programmer to manually enter the index and subindex values that they want to access. This requires the Banner IO-Link Master AOI to work. It is meant to support non-Banner IO-Link devices. It can also be used to if memory constraints of the PLC do not allow for the all in one AOIs (for Banner IO-Link Devices).