Release Notes

This document contains information on current and past releases of the Safety Controller PC Interface software.

Version 4.1.0 May 2019

**SC10 Safety Controller**

Added the following language options German, Spanish, French, Italian, Japanese, Korean, Portuguese, Chinese (Mainland), Chinese (Taiwan).

**SC26 and XS26 Series Safety Controllers**

No new features have been added since Version 3.3.0

Version 4.0.0 April 2019

**SC10 Safety Controller**

Initial launch of the SC10 product. Supports all features and functions as detailed in the Instruction Manual.

**SC26 and XS26 Series Safety Controllers**

No new features have been added since Version 3.3.0

Version 3.3.0 May 2018

**SC10 Safety Controller**

Not Applicable

**SC26 and XS26 Series Safety Controllers**

New Features

* Added delay state indication to function blocks and safety outputs in Live Mode.
* Added ability to toggle an input reference node in Simulation Mode.
* Added status output states in Functional View in Simulation Mode.
* Added milliseconds option to Muting Time Limit feature.

Version 3.2.0 and earlier

**For details on these versions, choose the Help button**  **on the toolbar of the PC Interface software. Then select the Release Notes option.**